ANNEX

CONTENTS
PART II
CHAPTER IV

Upper legform to bonnet leading edge tests

Notes
1.
Interpolate vertically between curves.
2.
With negative bumper leads — test as for zero bumper lead.
3.
With bumper leads above 150 mm — test as for 150 mm.
4.
With bonnet leading edge heights above 1 050 mm — test as for 1 050 mm.