Article 1
1
The product group ‘light sources’ shall comprise all light sources of a luminous flux ≥ 60 and ≤ 12 000 lumens for general lighting applications with direct or indirect connection to the public electricity supply equipped with a lamp cap listed in EN 60061 and made in order to produce a visible radiation.
2
The following types of light sources are not included in the product group: directional lamps, high-intensity discharge lamps, coloured lamps, projector lamps, photographic lighting, solarium tubes, battery driven systems and other light sources that are not intended for general lighting applications. The following types of light sources are not included in the product group if they are not supplied directly from the mains: integral compact fluorescent lamps, filament lamps, LED lamps.