Article 1
Subject matter
Article 2
Specification of the European register of authorised types of vehicles
Article 2a
Information to be inserted by the Agency
Article 3
Information to be sent by national safety authorities
Article 4
Restriction codes
Article 5
Final provisions
Article 6
Date of application
Article 7
Addressees
ANNEX I
SPECIFICATION FOR THE EUROPEAN REGISTER OF AUTHORISED TYPES OF VEHICLES
1.
TYPES OF VEHICLE TO BE VOLUNTARILY REGISTERED
2.
FUNCTIONAL ARCHITECTURE
2.1.
Administration of ERATV
2.2.
Address of ERATV
2.3.
Users and user access rights
2.4.
Interface to external systems
2.5.
Links to other registers and databases
2.6.
Availability
2.7.
Security
3.
TECHNICAL ARCHITECTURE
3.1.
System architecture
3.2.
System requirements
4.
OPERATING MODE
5.
RULES FOR DATA INPUT AND CONSULTATION
5.1.
General principle
5.2.
Submission of data by national safety authority
5.2.1.
Registering a new vehicle type authorisation, a new vehicle type...
(1)
The national safety authority shall inform the Agency of any...
(2)
The national safety authority shall inform the Agency of any...
(3)
The national safety authority shall inform the Agency of any...
(4)
The Agency shall check the information submitted by the national...
(5)
After validation of the information submitted by the national safety...
5.2.2.
Granting an authorisation to a type of vehicle previously registered...
5.2.3.
Modification on an existing authorisation
5.2.4.
Suspension
5.2.5.
Reactivation without modification
5.2.6.
Reactivation with modification
5.2.7.
Withdrawal
5.2.8.
Modification of an authorisation which may lead to a modification...
5.3.
Entry or modification of data by the Agency
5.3.1.
The authorising entity is a national safety authority
5.3.2.
The authorising entity is the Agency
5.4.
Publication of data by the Agency
5.5.
Error handling in submitted data
5.6.
Possible searches and reports
5.7.
Historical records
5.8.
Automatic notification of changes
6.
GLOSSARY
ANNEX II
DATA TO BE REGISTERED AND FORMAT
(1)
For each authorised type of vehicle, ERATV shall include the...
(2)
The data to be registered in ERATV for each type...
(3)
The values indicated for the parameters related to the technical...
(4)
In the cases where possible values for a parameter are...
(5)
For the types of vehicle that are not in conformity...
(6)
Where a parameter is defined in the applicable TSI, the...
(7)
Predefined lists shall be maintained and kept updated by the...
(8)
For parameters indicated as ‘ open point ’ no data...
(9)
For parameters indicated as ‘ optional ’ , indication of...
(10)
Fields 0.1-0.4 shall be filled in by the Agency.
ANNEX III
STRUCTURE OF TYPE NUMBER
Each type of vehicle shall receive a number consisting of...
XX XXX XXXX X Category — Family (Platform) Incrementa number...
Where:
Field 1 (digits 1 and 2) is assigned according to...
Code Category Subcategory 11 Traction vehicles Locomotive 12 Reserved 13...
Field 2 (digits from 3 to 5) is assigned according...
Field 3 (digits from 6 to 9) is a progressive...
Field 4 (digit 10) is a check digit determined in...
the digits in the even positions of the basic number...
Examples of determining the check digit:
1 —
Let the basic number be 3 3 8 4 4...
2 —
Let the basic number be 3 1 5 1 3...
If the type examination certificate or design examination certificate covers...
Commission Implementing Decision
of 4 October 2011
on the European register of authorised types of railway vehicles
(notified under document C(2011) 6974)
(Text with EEA relevance)
(2011/665/EU) (revoked)
. . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . .
Decision revoked (31.12.2020) by The Railways (Interoperability) (Miscellaneous Amendments and Revocations) (EU Exit) Regulations 2020 (S.I. 2020/318), reg. 1(2)(c), Sch. 2