Article 1
Decision 2012/88/EU is amended as follows:
1. Article 6 is deleted.
2. The following Article is inserted:
Article 6a
When implementing the TSI set out in Annex III to this Decision, one of the two sets of specifications listed in table A-2 of Annex A shall be applied. Baseline 3 specifications shall be maintained in order to ensure that trains equipped with Baseline 3-compliant ERTMS/ETCS can run on Baseline 2-compliant ERTMS/ETCS lines without any additional technical or operational restrictions.
3. Annex A is replaced by Annex I to this Decision.
4. Annex G is replaced by Annex II to this Decision