ANNEX
1.

GENERIC UWB USAGE
. . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . .
2.

LOCATION TRACKING SYSTEMS TYPE 1 (LT1)
. . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . .
3.

UWB DEVICES INSTALLED IN ROAD AND RAIL VEHICLES
. . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . .
4.

UWB ONBOARD AIRCRAFT
. . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . .
5.

MATERIAL SENSING DEVICES USING UWB TECHNOLOGY
5.1.

Material sensing devices
. . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . .
5.2.

Building material analysis devices (BMA)
1.

BMA Devices permitted under this Decision shall fulfil the following requirements:
. . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . .
2.

Emissions radiating from BMA devices shall be kept to a minimum and in any case not exceed the maximum power limits within the table below with the BMA device on a representative wall as defined within ETSI Standards EN 302 435-1 and EN 302 498-2.
. . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . .
Decision revoked (31.12.2020) by The Radio Spectrum (EU Exit) Regulations 2018 (S.I. 2018/1385), reg. 1, Sch. 2 para. 34; 2020 c. 1, Sch. 5 para. 1(1)