Article 1
1
The efficient exterior lighting system including low-beam headlamp, high-beam headlamp, front position, front fog, rear fog, front turn signal, rear turn signal, licence plate and reversing lamp fitted with light emitting diodes (LEDs) intended for use in M1 vehicles is approved as an innovative technology within the meaning of Article 12 of Regulation (EC) No 443/2009.
2
The CO2 emissions reduction from the use of the efficient exterior lighting system including all, or an appropriate combination of the lighting functions referred to in paragraph 1 shall be determined using the methodology set out in the Annex.
3
The individual eco-innovation code to be entered into type-approval documentation to be used for the innovative technology approved through this Implementing Decision shall be ‘15’.
Article 2. . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . .
Done at Brussels, 5 February 2016.
For the Commission
The President
Jean-Claude Juncker
Art. 2 omitted (31.12.2020) by virtue of The Road Vehicle Carbon Dioxide Emission Performance Standards (Cars and Vans) (Amendment) (EU Exit) Regulations 2019 (S.I. 2019/550), regs. 1, 19(2); 2020 c. 1, Sch. 5 para. 1(1)