Approval
Article 1
The BMW AG engine idle coasting function, hereinafter BMW engine idle coasting function, is approved as an innovative technology within the meaning of Article 12 of Regulation (EC) No 443/2009 provided the following conditions are met:
1. the innovative technology is fitted in BMW conventional powertrain M1 vehicles with automatic transmission equipped with the BMW engine idle coasting function automatically activated in the predominant driving mode; this is the driving mode that is always selected when the vehicle is switched on regardless of the operating mode selected when the vehicle was previously shut down; the BMW engine idle coasting function may not be deactivated in the predominant driving mode by the driver or by external interventions;
2. the BMW engine idle coasting function is active at least down to 40km/h;
3. for vehicles with the capacity to coast down to a speed lower than 40km/h, the BMW engine idle coasting function shall be de-activated at 40km/h for the purpose of the test set out in the Annex.