Stability requirements and phasing-out of ro-ro passenger ships
Article 7
1
Ro-ro passenger ships of Class C, the keels of which were laid or which were at a similar stage of construction on or after
1 October 2004
, and all ro-ro passenger ships of Classes A and B shall comply with Articles 6, 8 and 9 of Directive 2003/25/EC.
2 . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . .
Substituted by Directive (EU) 2017/2108 of the European Parliament and of the Council of 15 November 2017 amending Directive 2009/45/EC on safety rules and standards for passenger ships (Text with EEA relevance).
Deleted by Directive (EU) 2017/2108 of the European Parliament and of the Council of 15 November 2017 amending Directive 2009/45/EC on safety rules and standards for passenger ships (Text with EEA relevance).