CHAPTER 4

CONFORMITY OF THE EXPLOSIVE

Conformity assessment procedures
Article 20
For the assessment of the conformity of explosives the manufacturer shall follow one of the following procedures referred to in Annex III:
1. EU-type examination (Module B) and, at the choice of the manufacturer, any of the following:
  1. conformity to type based on internal production control plus supervised product checks at random intervals (Module C2);
  2. conformity to type based on quality assurance of the production process (Module D);
  3. conformity to type based on product quality assurance (Module E);
  4. conformity to type based on product verification (Module F);
2. conformity based on unit verification (Module G).