TITLE II

TOBACCO PRODUCTS
CHAPTER I

Ingredients and emissions

Measurement methods
Article 4
1
The tar, nicotine and carbon monoxide emissions from cigarettes shall be measured on the basis of ISO standard 4387 for tar, ISO standard 10315 for nicotine, and ISO standard 8454 for carbon monoxide.
The accuracy of the tar, nicotine and carbon monoxide measurements shall be determined in accordance with ISO standard 8243.
2
The measurements referred to in paragraph 1 shall be verified by laboratories which are approved and monitored by the competent authorities of the Member States.
Those laboratories shall not be owned or controlled directly or indirectly by the tobacco industry.
Member States shall communicate to the Commission a list of approved laboratories, specifying the criteria used for approval and the methods of monitoring applied, and shall update that list whenever any change is made. The Commission shall make those lists of approved laboratories publicly available.
3
The Commission shall be empowered to adopt delegated acts in accordance with Article 27 to adapt the methods of measurement of the tar, nicotine and carbon monoxide emissions, where this is necessary, based on scientific and technical developments or internationally agreed standards.
4
Member States shall notify the Commission of any measurement methods they use for emissions from cigarettes other than the emissions referred to in paragraph 3 and for emissions from tobacco products other than cigarettes.
5
The Commission shall adopt delegated acts in accordance with Article 27 to integrate standards agreed by the parties to the FCTC or by the WHO for measurement methods into Union law.
6
Member States may charge manufacturers and importers of tobacco products proportionate fees for the verification of the measurements referred to in paragraph 1 of this Article.