Article 1
In Annex III to Directive 2014/32/EU, point 1 is replaced by the following:
1.

The flowrate range of the water.
The values for the flowrate range shall fulfil the following conditions:
- Q3/Q1 ≥ 40
- Q2/Q1 = 1,6
- Q4/Q3 = 1,25
.