ANNEX I B

REQUIREMENTS FOR CONSTRUCTION, TESTING, INSTALLATION AND INSPECTION
Appendix 3

PICTOGRAMS
The recording equipment may optionally use the following pictograms and pictogram combinations (or pictograms and combination similar enough to be unambiguously identifiable with these):
1. BASIC PICTOGRAMS
| People | Actions | Modes of operation
| Company | | Company mode
| Controller | Control | Control mode
| Driver | Driver | Operational mode
| Workshop/test station | Inspection/calibration | Calibration mode
| Manufacturer | |
| Activities | Duration
| Available | Current availability period
| Driving | Continuous driving time
| Rest | Current rest period
| Work | Current work period
| Break | Cumulative break time
| Unknown |
| Equipment | Functions
| Driver slot |
| Co-driver slot |
| Card |
| Clock |
| Display | Displaying
| External storage | Downloading
| Power supply |
| Printer/printout | Printing
| Sensor |
| Tyre size |
| Vehicle/vehicle unit |
| Specific conditions
| Out of scope
| Ferry/train crossing
| Miscellaneous | |
| Events | | Faults
| Start of daily work period | | End of daily work period
| Location | | Manual entry of driver activities
| Security | | Speed
| Time | | Total/summary
| Qualifiers
| Daily
| Weekly
| Two weeks
| From or to
2. PICTOGRAM COMBINATIONS
| Miscellaneous | |
| Control place | |
| Location start of daily work period | | Location end of daily work period
| From time | | To time
| From vehicle | |
| Out of scope begin | | Out of scope end
| Cards
| Driver card
| Company card
| Control card
| Workshop card
- - - | No card
| Driving
| Crew driving
| Driving time for one week
| Driving time for two weeks
| Printouts
| Driver activities from card daily printout
| Driver activities from VU daily printout
| Events and faults from card printout
| Events and faults from VU printout
| Technical data printout
| Over speeding printout
| Events
| Insertion of a non valid card
| Card conflict
| Time overlap
| Driving without an appropriate card
| Card insertion while driving
| Last card session not correctly closed
| Over speeding
| Power supply interruption
| Motion data error
| Security breach
| Time adjustment (by workshop)
| Over speeding control
| Vehicle Motion Conflict
| Faults
| Card fault (driver slot)
| Card fault (co-driver slot)
| Display fault
| Downloading fault
| Printer fault
| Sensor fault
| VU internal fault
| Manual entries procedure
| Still same daily work period?
| End of previous work period?
| Confirm or enter location of end of work period
| Enter start time
| Enter location of start of work period.
Note: Additional pictogram combinations to form printout block or record identifiers are defined in Appendix 4.
PIC_001
Inserted by Council Regulation (EC) No 2135/98 of 24 September 1998 amending Regulation (EEC) No 3821/85 on recording equipment in road transport and Directive 88/599/EEC concerning the application of Regulations (EEC) No 3820/85 and (EEC) No 3821/85.
Substituted by Commission Regulation (EC) No 1360/2002 of 13 June 2002 adapting for the seventh time to technical progress Council Regulation (EEC) No 3821/85 on recording equipment in road transport (Text with EEA relevance).
Substituted by Commission Regulation (EU) No 1266/2009 of 16 December 2009 adapting for the tenth time to technical progress Council Regulation (EEC) No 3821/85 on recording equipment in road transport (Text with EEA relevance).
Inserted by Commission Regulation (EU) No 1266/2009 of 16 December 2009 adapting for the tenth time to technical progress Council Regulation (EEC) No 3821/85 on recording equipment in road transport (Text with EEA relevance).