ANNEX I B

REQUIREMENTS FOR CONSTRUCTION, TESTING, INSTALLATION AND INSPECTION
Appendix 5

DISPLAY
In this appendix the following format notation conventions have been used:
- characters printed in
bold
denote plain text to be displayed (display remains in normal character),
- normal characters denote variables (pictograms or data) to be replaced by their values for displaying:
dd mm yyyy
  - day, month, year,
hh
  - hours,
mm
  - minutes,
D
  - duration pictogram,
EF
  - event or fault pictograms combination,
O
  - mode of operation pictogram.
The recording equipment shall display data using the following formats:
Data | Format
Default display
Local time | hh:mm
Mode of operation | O
Information related to the driver | Dhhhmm hhhmm
Information related to the co-driver | Dhhh mm
Out of scope condition opened |
Warning display
Exceeding continuous driving time | hhhmm hhh mm
Event or fault | EF
Other displays
UTC date | UTC dd/mm/yyyy or UTC dd.mm.yyyy
time | hh:mm
Driver's continuous driving time and cumulative break time | hhhmm hhh mm
Co-driver's continuous driving time and cumulative break time | hhh mm hhh mm
Driver's cumulated driving time for the previous and the current week | hhhh mm
Co-driver's cumulated driving time for the previous and the current week | hhhh mm
DIS_001
Inserted by Council Regulation (EC) No 2135/98 of 24 September 1998 amending Regulation (EEC) No 3821/85 on recording equipment in road transport and Directive 88/599/EEC concerning the application of Regulations (EEC) No 3820/85 and (EEC) No 3821/85.
Substituted by Commission Regulation (EC) No 1360/2002 of 13 June 2002 adapting for the seventh time to technical progress Council Regulation (EEC) No 3821/85 on recording equipment in road transport (Text with EEA relevance).