Application for EC type-approval of a vehicle with regard to emissions and access to vehicle repair and maintenance information
Article 5
1
The manufacturer shall submit to the approval authority an application for EC type-approval of a vehicle with regard to emissions and access to vehicle repair and maintenance information.
2
The application referred to in paragraph 1 shall be drawn up in accordance with the model of the information document set out in Appendix 3 to Annex I.
3
In addition, the manufacturer shall submit the following information:
a
in the case of vehicles equipped with positive-ignition engines, a declaration by the manufacturer of the minimum percentage of misfires out of a total number of firing events that either would result in emissions exceeding the limits given in section 2.3 of Annex XI if that percentage of misfire had been present from the start of a type 1 test as described in Annex III to this Regulation or could lead to an exhaust catalyst, or catalysts, overheating prior to causing irreversible damage;
b
detailed written information fully describing the functional operation characteristics of the OBD system, including a listing of all relevant parts of the emission control system of the vehicle that are monitored by the OBD system;
c
a description of the malfunction indicator used by the OBD system to signal the presence of a fault to a driver of the vehicle;
d
a declaration by the manufacturer that the OBD system complies with the provisions of section 3 of Appendix 1 to Annex XI relating to in-use performance under all reasonably foreseeable driving conditions;
e
a plan describing the detailed technical criteria and justification for incrementing the numerator and denominator of each monitor that must fulfil the requirements of sections 3.2 and 3.3 of Appendix 1 to Annex XI, as well as for disabling numerators, denominators and the general denominator under the conditions outlined in section 3.7 of Appendix 1 to Annex XI;
f
a description of the provisions taken to prevent tampering with and modification of the emission control computer;
g
if applicable, the particulars of the vehicle family as referred to in Appendix 2 to Annex XI;
h
where appropriate, copies of other type-approvals with the relevant data to enable extension of approvals and establishment of deterioration factors.
4
For the purposes of paragraph 3(d), the manufacturer shall use the model of a manufacturer’s certificate of compliance with the OBD in-use performance requirements set out in Appendix 7 of Annex I
5
For the purposes of paragraph 3(e), the approval authority that grants the approval shall make the information referred to in that point available to the approval authorities or the Commission upon request.
6
For the purposes of points (d) and (e) of paragraph 3, approval authorities shall not approve a vehicle if the information submitted by the manufacturer is inappropriate for fulfilling the requirements of section 3 of Appendix 1 to Annex XI.
Sections 3.2, 3.3 and 3.7 of Appendix 1 to Annex XI shall apply under all reasonably foreseeable driving conditions.
For the assessment of the implementation of the requirements set out in the first and second subparagraphs, the approval authorities shall take into account the state of technology.
7
For the purposes of paragraph 3(f), the provisions taken to prevent tampering with and modification of the emission control computer shall include the facility for updating using a manufacturer-approved programme or calibration.
8
For the tests specified in Figure I.2.4 of Annex I the manufacturer shall submit to the technical service responsible for the type-approval tests a vehicle representative of the type to be approved.
9
The application for type-approval of mono fuel, bi-fuel and flex-fuel vehicles shall comply with the additional requirements laid down in Sections 1.1 and 1.2 of Annex I.
10
Changes to the make of a system, component or separate technical unit that occur after a type-approval shall not automatically invalidate a type approval, unless its original characteristics or technical parameters are changed in such a way that the functionality of the engine or pollution control system is affected.
11
The manufacturer shall also provide an extended documentation package with the following information:
a
information on the operation of all AES and BES, including a description of the parameters that are modified by any AES and the boundary conditions under which the AES operate, and indication of the AES or BES which are likely to be active under the conditions of the test procedures set out in this Regulation;
b
a description of the fuel system control logic, timing strategies and switch points during all modes of operation.
12
The extended documentation package referred to in paragraph 11 shall remain strictly confidential. It may be kept by the approval authority, or, at the discretion of the approval authority, may be retained by the manufacturer. In the case the manufacturer retains the documentation package, that package shall be identified and dated by the approval authority once reviewed and approved. It shall be made available for inspection by the approval authority at the time of approval or at any time during the validity of the approval.
Inserted by Commission Regulation (EU) 2016/646 of 20 April 2016 amending Regulation (EC) No 692/2008 as regards emissions from light passenger and commercial vehicles (Euro 6) (Text with EEA relevance).