Article 1
Regulation (EC) No 1272/2008 is amended as follows:
1. Article 25(5) is deleted;
2. the following new section (e) is inserted in Article 26(1):
  1. if the hazard pictogram “GHS02” or “GHS06” applies, the use of the hazard pictogram “GHS04” shall be optional.
;
3. Annex I is amended in accordance with Annex I to this Regulation;
4. Annex II is amended in accordance with Annex II to this Regulation;
5. Annex III is amended in accordance with Annex III to this Regulation;
6. Annex IV is amended in accordance with Annex IV to this Regulation;
7. Annex V is amended in accordance with Annex V to this Regulation;
8. Annex VI is amended in accordance with Annex VI to this Regulation;
9. Annex VII is amended in accordance with Annex VII to this Regulation.