Provisions for GB type-approval of a type of vehicle with regard to its masses and dimensions
Article 4
1
The manufacturer or his representative shall submit to the type-approval authority the application for GB type-approval of a type of vehicle as regard its masses and dimensions.
2
The application shall be drawn up in accordance with the model information document set out in Part A of Annex V.
3
For the purposes of mass distribution calculations, the manufacturer shall provide the type-approval authority, for each technical configuration within the vehicle type as determined by the set of values of the relevant points in Annex V, with the information necessary to identify the following masses:
a
the technically permissible maximum laden mass;
b
the technically permissible maximum mass on the axles or group of axles;
c
the technically permissible maximum towable mass;
d
the technically permissible maximum mass at the coupling point(s);
e
the technically permissible maximum laden mass of the combination.
The information shall be provided in tabular or any other appropriate format, in agreement with the type-approval authority.
4
Where the optional equipment significantly affects the masses and dimensions of the vehicle, the manufacturer shall provide the technical service with the location, mass and geometrical position of the gravity centre with respect to the axles of the optional equipment that can be fitted to the vehicle.
5
By way of derogation from paragraph 4, where the optional equipment is made up of several parts located in various spaces in the vehicle, the manufacturer may provide the technical service with the distribution of the mass of the optional equipment on the axles only.
6
For groups of axles, the manufacturer shall indicate the load distribution among the axles of the total mass applied to the group.
Where necessary, the manufacturer shall state the distribution formulae or produce the relevant distribution graphs.
7
Where the approval authority or the technical service deems it necessary, they may request the manufacturer to make available a vehicle representative of the type to be approved for the purposes of inspection.
8
The vehicle manufacturer may submit an application for recognition of the equivalence of a suspension to air suspension to the type-approval authority.
The type-approval authority shall recognise the equivalence of a suspension to air suspension where the requirements of Annex III are fulfilled.
Where the technical service has recognised the equivalence, it shall issue a test report. The type-approval authority shall attach the test report and a technical description of the suspension to the GB type-approval certificate.
9
Where the requirements set out in Annexes I to IV, of this Regulation are met, the approval authority shall grant a GB type-approval in accordance with the numbering system set out in Annex IV to Commission Implementing Regulation (EU) 2020/683.
The approval authority shall not assign the same number to another vehicle type.
10
For the purposes of paragraph 9, the type-approval authority shall deliver a GB type-approval certificate established in accordance with the model set out in Part B of Annex V.
11
The permissible deviations referred to in Appendix 2 to Annex I shall apply for the purposes of Article 31(3) and (4) of Regulation (EU) 2018/858
Words in Art. 4 heading substituted (31.12.2022 at 11.00 p.m.) by The Road Vehicles and Non-Road Mobile Machinery (Type-Approval) (Amendment and Transitional Provisions) (EU Exit) Regulations 2022 (S.I. 2022/1273), regs. 1(2), 71(4)(a)
Words in Art. 4(1) substituted (31.12.2022 at 11.00 p.m.) by The Road Vehicles and Non-Road Mobile Machinery (Type-Approval) (Amendment and Transitional Provisions) (EU Exit) Regulations 2022 (S.I. 2022/1273), regs. 1(2), 71(4)(a)
Words in Art. 4(8) substituted (31.12.2022 at 11.00 p.m.) by The Road Vehicles and Non-Road Mobile Machinery (Type-Approval) (Amendment and Transitional Provisions) (EU Exit) Regulations 2022 (S.I. 2022/1273), regs. 1(2), 71(4)(a)
Word in Art. 4(9) inserted (31.12.2022 at 11.00 p.m.) by The Road Vehicles and Non-Road Mobile Machinery (Type-Approval) (Amendment and Transitional Provisions) (EU Exit) Regulations 2022 (S.I. 2022/1273), regs. 1(2), 71(4)(b)(i)(aa)
Words in Art. 4(9) substituted (31.12.2022 at 11.00 p.m.) by The Road Vehicles and Non-Road Mobile Machinery (Type-Approval) (Amendment and Transitional Provisions) (EU Exit) Regulations 2022 (S.I. 2022/1273), regs. 1(2), 71(4)(b)(i)(bb)
Words in Art. 4(9) substituted (31.12.2022 at 11.00 p.m.) by The Road Vehicles and Non-Road Mobile Machinery (Type-Approval) (Amendment and Transitional Provisions) (EU Exit) Regulations 2022 (S.I. 2022/1273), regs. 1(2), 71(4)(b)(ii)
Words in Art. 4(10) substituted (31.12.2022 at 11.00 p.m.) by The Road Vehicles and Non-Road Mobile Machinery (Type-Approval) (Amendment and Transitional Provisions) (EU Exit) Regulations 2022 (S.I. 2022/1273), regs. 1(2), 71(4)(c)
Words in Art. 4(11) substituted (31.12.2022 at 11.00 p.m.) by The Road Vehicles and Non-Road Mobile Machinery (Type-Approval) (Amendment and Transitional Provisions) (EU Exit) Regulations 2022 (S.I. 2022/1273), regs. 1(2), 71(4)(d)