Subject matter and scope
Article 1
1
This Regulation establishes ecodesign requirements for the placing on the market of rotodynamic water pumps for pumping clean water, including where integrated in other products.
2
This Regulation shall not apply to:
a
water pumps designed specifically for pumping clean water at temperatures below – 10 °C or above 120 °C, except with regard to the information requirements of Annex II, points 2(11) to 2(13);
b
water pumps designed only for fire-fighting applications;
c
displacement water pumps;
d
self-priming water pumps.