CHAPTER III

MONITORING OF EMISSIONS OF STATIONARY INSTALLATIONS
SECTION 1

General provisions

Choice of the monitoring methodology
Article 21
1
For the monitoring of the emissions of an installation, the operator shall choose to apply either a calculation-based methodology or a measurement-based methodology, subject to specific provisions of this Regulation.
A calculation-based methodology shall consist in determining emissions from source streams based on activity data obtained by means of measurement systems and additional parameters from laboratory analyses or default values. The calculation-based methodology may be implemented through the standard methodology set out in Article 24 or the mass balance methodology set out in Article 25.
A measurement-based methodology shall consist in determining emissions from emission sources by means of continuous measurement of the concentration of the relevant greenhouse gas in the flue gas and of the flue gas flow, including the monitoring of CO2 transfers between installations where the CO2 concentration and the flow of the transferred gas are measured.
Where the calculation-based methodology is applied, the operator shall for each source stream define, in the monitoring plan, whether the standard methodology or the mass balance methodology is used, including the relevant tiers in accordance with Annex II.
2
An operator may combine, subject to approval by the competent authority, standard methodology, mass balance and measurement-based methodologies for different emission sources and source streams belonging to one installation, provided that neither gaps nor double counting concerning emissions occur.
3
Where the operator does not choose a measurement-based methodology, the operator shall choose the methodology required by the relevant section of Annex IV, unless he provides evidence to the competent authorities that the use of such methodology is technically not feasible or incurs unreasonable costs, or that another methodology leads to a higher overall accuracy of emissions data.