CHAPTER III

MONITORING OF EMISSIONS OF STATIONARY INSTALLATIONS
SECTION 1

General provisions

Monitoring methodology not based on tiers
Article 22
By way of derogation from Article 21(1), the operator may use a monitoring methodology that is not based on tiers (hereinafter ‘the fall-back methodology’) for selected source streams or emission sources, provided that all of the following conditions are met:
1. applying at least tier 1 under the calculation-based methodology for one or more major source streams or minor source streams and a measurement-based methodology for at least one emission source related to the same source streams is technically not feasible or would incur unreasonable costs;
2. the operator assesses and quantifies each year the uncertainties of all parameters used for the determination of the annual emissions in accordance with the ISO Guide to the Expression of Uncertainty in Measurement (JCGM 100:2008), or another equivalent internationally accepted standard, and includes the results in the annual emissions report;
3. the operator demonstrates to the satisfaction of the competent authority that by applying such a fall-back monitoring methodology, the overall uncertainty thresholds for the annual level of greenhouse gas emissions for the whole installation do not exceed 7,5 % for category A installations, 5,0 % for category B installations and 2,5 % for category C installations.