CHAPTER III

MONITORING OF EMISSIONS OF STATIONARY INSTALLATIONS
SECTION 2

Calculation-based methodology
Subsection 1

General

Applicable tiers
Article 26
1
When defining the relevant tiers in accordance with Article 21(1), to determine the activity data and each calculation factor, each operator shall apply the following:
a
at least the tiers listed in Annex V, in the case of an installation that is a category A installation, or where a calculation factor is required for a source stream that is a commercial standard fuel;
b
in other cases than those referred to in point (a), the highest tier as defined in Annex II.
However, the operator may apply a tier one level lower than required in accordance with the first subparagraph for category C installations and up to two levels lower for category A and B installations, with a minimum of tier 1, where it shows to the satisfaction of the competent authority that the tier required in accordance with the first subparagraph is technically not feasible or incurs unreasonable costs.
The competent authority may, for a transitional period of up to three years, allow an operator to apply lower tiers than those referred to in the second subparagraph, with a minimum of tier 1, provided that both of the following conditions are met:
a
the operator shows to the satisfaction of the competent authority that the tier required pursuant to the second subparagraph is technically not feasible or incurs unreasonable costs;
b
the operator provides an improvement plan indicating how and by when at least the tier required pursuant to the second subparagraph will be reached.
2
For activity data and each calculation factor for minor source streams, the operator shall apply the highest tier which is technically feasible and does not incur unreasonable costs, with a minimum of tier 1.
3
For activity data and each calculation factor for de-minimis source streams, the operator may determine activity data and each calculation factor by using conservative estimations instead of using tiers, unless a defined tier is achievable without additional effort.
4
For the oxidation factor and conversion factor, the operator shall, as a minimum, apply the lowest tiers listed in Annex II.
5
Where the competent authority has allowed the use of emission factors expressed as t CO2/t or t CO2/Nm3 for fuels, and for fuels used as process input or in mass balances in accordance with Article 25, the net calorific value may be monitored using lower tiers than the highest tier as defined in Annex II.