CHAPTER III

MONITORING OF EMISSIONS OF STATIONARY INSTALLATIONS
SECTION 2

Calculation-based methodology
Subsection 2

Activity data

Measurement systems under the operator’s control
Article 28
1
For determining the activity data in accordance with Article 27, the operator shall use metering results based on measurement systems under its own control at the installation, provided that all of the following conditions are complied with:
a
the operator must carry out an uncertainty assessment and ensures that the uncertainty threshold of the relevant tier level is met;
b
the operator must ensure at least once per year, and after each calibration of measuring instruments, that the calibration results multiplied by a conservative adjustment factor based on an appropriate time series of previous calibrations of that or similar measuring instruments for taking into account the effect of uncertainty in service, are compared with the relevant uncertainty thresholds.
Where tier thresholds approved in accordance with Article 12 are exceeded or equipment found not to conform to other requirements, the operator shall take corrective action without undue delay and notify the competent authority thereof.
2
The operator shall provide the uncertainty assessment referred to in point (a) of paragraph 1 to the competent authority when notifying a new monitoring plan or when it is relevant for a change to the approved monitoring plan.
The assessment shall comprise the specified uncertainty of the applied measuring instruments, uncertainty associated with the calibration, and any additional uncertainty connected to how the measuring instruments are used in practice. Uncertainty related to stock changes shall be included in the uncertainty assessment where the storage facilities are capable of containing at least 5 % of the annual used quantity of the fuel or material considered. When carrying out the assessment, the operator shall take into account the fact that the stated values used to define tier uncertainty thresholds in Annex II refer to the uncertainty over the full reporting period.
The operator may simplify the uncertainty assessment by assuming that the maximum permissible errors specified for the measuring instrument in service, or where lower, the uncertainty obtained by calibration, multiplied by a conservative adjustment factor for taking into account the effect of uncertainty in service, is to be regarded as the uncertainty over the whole reporting period as required by the tier definitions in Annex II, provided that measuring instruments are installed in an environment appropriate for their use specifications.
3
Notwithstanding paragraph 2, the competent authority may allow the operator to use metering results based on measurement systems under its own control at the installation, where the operator provides evidence that the measuring instruments applied are subject to relevant national legal metrological control.
For that purpose, the maximum permissible error in service allowed by the relevant national legislation on legal metrological control for the relevant measuring task may be used as the uncertainty value without providing further evidence.