CHAPTER III

MONITORING OF EMISSIONS OF STATIONARY INSTALLATIONS
SECTION 2

Calculation-based methodology
Subsection 3

Calculation factors

Determination of calculation factors
Article 30
1
The operator shall determine calculation factors either as default values or values based on analysis depending on the applicable tier.
2
The operator shall determine and report calculation factors consistently with the state used for related activity data, referring to the fuel’s or material’s state in which the fuel or material is purchased or used in the emission causing process, before it is dried or otherwise treated for laboratory analysis.
Where such an approach incurs unreasonable costs, or where higher accuracy can be achieved, the operator may consistently report activity data and calculation factors referring to the state in which laboratory analyses are carried out.