CHAPTER III

MONITORING OF EMISSIONS OF STATIONARY INSTALLATIONS
SECTION 2

Calculation-based methodology
Subsection 3

Calculation factors

Frequencies for analyses
Article 35
1
The operator shall apply the minimum frequencies for analyses for relevant fuels and materials listed in Annex VII. Annex VII will be reviewed on a regular basis and in the first instance not more than two years from this Regulation entering into force.
2
The competent authority may allow the operator to use a different frequency than those referred to in paragraph 1, where minimum frequencies are not available or where the operator demonstrates one of the following:
a
based on historical data, including analytical values for the respective fuels or materials in the reporting period immediately preceding the current reporting period, any variation in the analytical values for the respective fuel or material does not exceed 1/3 of the uncertainty value to which the operator has to adhere with regard to the activity data determination of the relevant fuel or material;
b
using the required frequency would incur unreasonable costs.