CHAPTER III

MONITORING OF EMISSIONS OF STATIONARY INSTALLATIONS
SECTION 3

Measurement-based methodology

Corroborating with calculation of emissions
Article 46
The operator shall corroborate emissions determined by a measurement-based methodology, with the exception of nitrous oxide (N2O) emissions from nitric acid production and greenhouse gases transferred to a transport network or a storage site, by calculating the annual emissions of each considered greenhouse gas for the same emission sources and source streams.
The use of tier methodologies shall not be required.