CHAPTER IV

MONITORING OF EMISSIONS AND TONNE-KILOMETRE DATA FROM AVIATION

Sources of uncertainty
Article 55
1
The aircraft operator shall consider sources of uncertainty and their associated levels of uncertainty when selecting the monitoring methodology pursuant to Article 52(2).
2 . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . .
3 . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . .
4 . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . .
5
The aircraft operator shall regularly perform suitable control activities, including cross-checks between the fuel uplift quantity as provided by invoices and the fuel uplift quantity indicated by on-board measurement, and take corrective action if notable deviations are observed.
Substituted by Commission Implementing Regulation (EU) 2018/2066 of 19 December 2018 on the monitoring and reporting of greenhouse gas emissions pursuant to Directive 2003/87/EC of the European Parliament and of the Council and amending Commission Regulation (EU) No 601/2012 (Text with EEA relevance).
Deleted by Commission Implementing Regulation (EU) 2018/2066 of 19 December 2018 on the monitoring and reporting of greenhouse gas emissions pursuant to Directive 2003/87/EC of the European Parliament and of the Council and amending Commission Regulation (EU) No 601/2012 (Text with EEA relevance).