Ecodesign requirements and timetable
Article 3
1
The ecodesign requirements for heaters are set out in Annex II.
2
Each ecodesign requirements shall apply in accordance with the following timetable:
a
from 26 September 2015:
1. heaters shall meet the requirements set out in Annex II, points 1(a), 3 and 5;
2. combination heaters shall meet the requirements set out in Annex II, point 2(a);
b
from 26 September 2017:
1. electric space heaters, electric combination heaters, cogeneration space heaters, heat pump space heaters and heat pump combination heaters shall meet the requirements set out in Annex II, point 1(b);
2. combination heaters shall meet the requirements set out in Annex II, point 2(b);
c
from 26 September 2018 heaters shall meet the requirements set out in Annex II, point 4(a).
3
Compliance with ecodesign requirements shall be measured and calculated in accordance with the requirements set out in Annex III.