Commission Regulation (EU) 2015/1189
of 28 April 2015
implementing Directive 2009/125/EC of the European Parliament and of the Council with regard to ecodesign requirements for solid fuel boilers
(Text with EEA relevance)
THE EUROPEAN COMMISSION,
Having regard to the Treaty on the Functioning of the European Union,
Having regard to Directive 2009/125/EC of the European Parliament and of the Council of 21 October 2009 establishing a framework for the setting of ecodesign requirements for energy-related products , and in particular Article 15(1) thereof,
After consulting the Consultation Forum referred to in Article 18 of Directive 2009/125/EC,
Whereas:
(1)
Directive 2009/125/EC requires the Commission to set ecodesign requirements for energy-related products that represent significant volumes of sales and trade, that have a significant environmental impact and that present significant potential for improvement in terms of their environmental impact without entailing excessive costs.
(2)
Article 16(2) of Directive 2009/125/EC provides that in accordance with the procedure referred to in Article 19(3) and the criteria set out in Article 15(2), and after consulting the Consultation Forum, the Commission should, if appropriate, introduce implementing measures for products offering a high potential for cost-effective reduction of greenhouse gas emissions, such as heating equipment, including solid fuel boilers and packages of a solid fuel boiler, supplementary heaters, temperature controls and solar devices.
(3)
The Commission has carried out a preparatory study to analyse the technical, environmental and economic aspects of the solid fuel boilers typically used in households and for commercial purposes. The study has been carried out with stakeholders and interested parties from the Union and third countries, and the results have been made publicly available.
(4)
The environmental aspects of solid fuel boilers that have been identified as significant for the purposes of this Regulation are energy consumption in the use phase and emissions of particulate matter (dust), organic gaseous compounds, carbon monoxide and nitrogen oxides in the use phase. The annual energy consumption related to solid fuel boilers is expected to be 530 petajoules (‘PJ’) (approximately 12,7 million tonnes of oil equivalent ‘Mtoe’) in 2030 and annual emissions are expected to be 25 kilotonnes (‘kt’) of particulate matter, 25 kt of organic gaseous compounds and 292 kt of carbon monoxide in 2030. Emissions of nitrogen oxides are expected to increase because of potential new solid fuel boiler designs aiming at higher energy efficiency and lower organic emissions. The preparatory study shows that use-phase energy consumption and emissions by solid fuel boilers can be significantly reduced.
(5)
The preparatory study shows that further requirements regarding ecodesign parameters for products referred to in Part 1 of Annex I to Directive 2009/125/EC are not necessary in the case of solid fuel boilers. In particular, emissions of dioxins and furans are not identified as significant.
(6)
Boilers generating heat exclusively for providing hot drinking or sanitary water, boilers for heating and distributing gaseous heat transfer media and cogeneration boilers with an electrical capacity of 50 kW or more have specific technical characteristics and should therefore be exempted from this Regulation. Non-woody biomass boilers are exempted, because at present there is insufficient European-wide information to determine appropriate levels for the ecodesign requirements for them and they may have further significant environmental impacts, such as furan and dioxin emissions. The appropriateness of setting ecodesign requirements for non-woody boilers will be reassessed when reviewing this Regulation.
(7)
The energy consumption and emissions of solid fuel boilers could be reduced by applying existing non-proprietary technologies without an increase in the combined costs of purchasing and operating these products.
(8)
The combined effect of the ecodesign requirements set out in this Regulation and Commission Delegated Regulation (EU) 2015/1187 is estimated to result by 2030 in annual energy savings of approximately 18 PJ (approximately 0,4 Mtoe), together with related carbon dioxide (‘CO2’) emission reductions of approximately 0,2 Mt, and a reduction of 10 kt in particulate matter, 14 kt in organic gaseous compounds, and 130 kt in carbon monoxide.
(9)
Ecodesign requirements should harmonise energy consumption and emission requirements for solid fuel boilers throughout the Union, for the internal market to operate better and in order to improve the environmental performance of those products.
(10)
The ecodesign requirements should not affect the functionality or affordability of solid fuel boilers from the end-user's perspective and should not negatively affect health, safety or the environment.
(11)
The introduction of ecodesign requirements should give manufacturers sufficient time to redesign their products subject to this Regulation. The timing should take into account the impact on manufacturers' costs, in particular for small and medium-sized enterprises, while ensuring timely achievement of the objectives of this Regulation.
(12)
Product parameters should be measured and calculated using reliable, accurate and reproducible methods which take into account recognised state-of-the-art measurement and calculation methods, including, where available, harmonised standards adopted by the European standardisation organisations following a request by the Commission, in accordance with the procedures laid down in Regulation (EU) No 1025/2012 of the European Parliament and of the Council .
(13)
In accordance with Article 8 of Directive 2009/125/EC, this Regulation specifies which conformity assessment procedures apply. While it is appropriate to review the appropriateness of third party certification at the same time as required by Commission Regulation (EU) No 813/2013 it is neither desirable nor seems feasible to make changes to the conformity assessment of solid fuel boilers before the entry into force of the ecodesign requirements.
(14)
In order to facilitate compliance checks, manufacturers should provide the information contained in the technical documentation referred to in Annexes IV and V to Directive 2009/125/EC insofar as that information relates to the requirements laid down in this Regulation.
(15)
To further limit the environmental impact of solid fuel boilers, manufacturers should provide information on disassembly, recycling and disposal.
(16)
In addition to the legally binding requirements laid down in this Regulation, indicative benchmarks for best available technologies should be determined to ensure that information on the life-cycle environmental performance of solid fuel boilers is widely available and easily accessible.
(17)
The measures provided for in this Regulation are in accordance with the opinion of the Committee established under Article 19(1) of Directive 2009/125/EC,
HAS ADOPTED THIS REGULATION:
OJ L 285, 31.10.2009, p. 10.
Commission Delegated Regulation (EU) 2015/1187 of 27 April 2015 supplementing Directive 2010/30/EU of the European Parliament and of the Council with regard to energy labelling of solid fuel boilers and packages of a solid fuel boiler, supplementary heaters, temperature controls and solar devices (see page 43 of this Official Journal)
Regulation (EU) No 1025/2012 of the European Parliament and of the Council of 25 October 2012 on European standardisation (OJ L 316, 14.11.2012, p. 12).
Commission Regulation (EU) No 813/2013 of 2 August 2013 implementing Directive 2009/125/EC of the European Parliament and of the Council with regard to ecodesign requirements for space heaters and combination heaters (OJ L 239, 6.9.2013, p. 136).