Commission Regulation (EU) 2015/166
of 3 February 2015
supplementing and amending Regulation (EC) No 661/2009 of the European Parliament and of the Council as regards the inclusion of specific procedures, assessment methods and technical requirements, and amending Directive 2007/46/EC of the European Parliament and of the Council, and Commission Regulations (EU) No 1003/2010, (EU) No 109/2011 and (EU) No 458/2011
(Text with EEA relevance)
THE EUROPEAN COMMISSION,
Having regard to the Treaty on the Functioning of the European Union,
Having regard to Directive 2007/46/EC of the European Parliament and of the Council of 5 September 2007 establishing a framework for the approval of motor vehicles and their trailers, and of systems, components and separate technical units intended for such vehicles (Framework Directive) , and in particular Article 39(2) thereof,
Having regard to Regulation (EC) No 661/2009 of the European Parliament and of the Council of 13 July 2009 concerning type-approval requirements for the general safety of motor vehicles, their trailers and systems, components and separate technical units intended therefor , and in particular Article 14(1)(a) and (f) thereof,
Whereas:
(1)
It is necessary to lay down detailed provisions for the type-approval of motor vehicles, their trailers and systems, components and separate technical units intended therefor regarding their general safety and to clarify the conditions of application of the relevant legislation made compulsory by Regulation (EC) No 661/2009.
(2)
Without prejudice to the list of regulatory acts setting the requirements for the purpose of EC type-approval of vehicles laid down in Annex IV to Directive 2007/46/EC, Regulation (EC) No 661/2009 provides vehicle manufacturers with the possibility to submit an application for type-approval for measures implementing Regulation (EC) No 661/2009 setting out requirements in areas covered by UNECE regulations.
(3)
It is in particular necessary to set out specific procedures for type-approval according to Article 20 of Directive 2007/46/EC concerning new technologies or concepts incompatible with the existing measures implementing Regulation (EC) No 661/2009 covered by UNECE regulations, as such provisions are currently unavailable, but needed.
(4)
It is in principle not possible to obtain type-approval in accordance with UNECE regulations in the case of installed components or separate technical units which have only a valid EC type-approval. However, this should be made possible for the purposes of EC type-approval according to Regulation (EC) No 661/2009, based on the provisions of the UNECE regulations.
(5)
Annex XV to Directive 2007/46/EC lists regulatory acts for which a manufacturer may be designated as technical service, including a number of Directives that are repealed by Regulation (EC) No 661/2009. It is therefore necessary to replace the references to the relevant Directives with references to the appropriate measures implementing Regulation (EC) No 661/2009.
(6)
Annex XVI to Directive 2007/46/EC lists the regulatory acts for which virtual testing may be used by the manufacturer or a technical service, including a number of Directives that are repealed by Regulation (EC) No 661/2009. It is therefore necessary to replace the relevant references to the relevant Directives with the references to the appropriate measures implementing Regulation (EC) No 661/2009.
(7)
To allow for a consistent approach with regard to the numbering of EC type-approval certificates and EC type-approval marks, it is further necessary to set out specific administrative provisions as well as a numbering and marking system under Regulation (EC) No 661/2009.
(8)
UNECE regulations contain specific provisions on the particulars that must accompany an application for type approval. In the context of the procedures provided for in this Regulation, those particulars should equally be indicated in the information folder.
(9)
Compliance with Council Directive 71/320/EEC , repealed by Regulation (EC) No 661/2009, is still compulsory for replacement brake lining assemblies but compliance with UNECE Regulation No 90 was accepted as an alternative. Detailed provisions, including adequate transitional provisions, have to be provided for regarding the replacement of brake lining assemblies, drum brake linings, brake discs and brake drums for power-driven vehicles and their trailers in accordance with UNECE Regulation No 90.
(10)
Concerning vehicles of category N, pursuant to Article 6(4) of Regulation (EC) No 661/2009, the vehicle cab or the space provided for the driver and passengers must be of sufficient strength to offer protection to the occupants in the event of an impact, taking account of UNECE Regulation No 29 . For this purpose, this regulation is to be included in the list of UNECE regulations which comply on a compulsory basis.
(11)
The table in Annex I to Regulation (EC) No 661/2009 laying down the scope of application for the requirements referred to in Article 5(1) and (2) of that Regulation needs to be updated following the adoption of Commission Directive 2010/19/EU .
(12)
Additional requirements concerning cab strength, tyre-pressure monitoring, advanced emergency braking, lane departure warning, gear shift indicator and electronic stability control set out in Regulation (EC) No 661/2009 are not incorporated in the table in Annex I, but should still apply for the purposes of type-approval.
(13)
The list of UNECE regulations which apply on a compulsory basis in Annex IV to Regulation (EC) No 661/2009 is updated frequently to reflect the current situation concerning amendments made to the respective UNECE regulations.
(14)
That list should be complemented with information clarifying under what conditions existing EC type-approvals granted on the basis of Directives repealed by Regulation (EC) No 661/2009 continue to be valid for certain vehicles, components and separate technical units.
(15)
Commission Regulation (EU) No 1003/2010 concerning the space for mounting and the fixing of rear registration plates needs to be revised to take account of specific vehicle designs.
(16)
Commission Regulation (EU) No 109/2011 concerning spray suppression systems needs to be amended to update the reference to the Commission Regulation on wheel guards as well as the latter being applicable for additional vehicle categories.
(17)
Commission Regulation (EU) No 458/2011 concerning the installation of tyres needs to be adapted to technical progress concerning the optional spare wheel for N1 category vehicles laid down in UNECE Regulation No 64 .
(18)
Two items in Annex XI to Directive 2007/46/EC listing regulatory acts for special purpose vehicles need to be revised with respect to vehicle sound level requirements so as to bring the applicable requirements back in conformity with provisions that were applied previously.
(19)
The measures provided for in this Regulation are in accordance with the opinion of the Technical Committee — Motor Vehicles,
HAS ADOPTED THIS REGULATION:

Subject matter
Article 1
1
This Regulation lays down detailed rules concerning the specific procedures, technical requirements and tests for the type-approval of vehicles of categories M, N and O, as well as components and separate technical units intended for such vehicles.
2
This Regulation also amends certain Annexes to Directive 2007/46/EC to adapt them to technical progress and to provide for procedures allowing type-approval:
- of new technologies or concepts in accordance with Article 20 of Directive 2007/46/EC,
- of vehicle systems in cases where components and separate technical units bearing an EC type-approval mark are applied instead of an ECE type-approval mark in the context of measures implementing Regulation (EC) No 661/2009 setting out requirements in areas covered by UNECE regulations,
- in cases where a manufacturer is designated as technical service in accordance with Annex XV to Directive 2007/46/EC, and
- in cases where virtual testing in accordance with Annex XVI to Directive 2007/46/EC has been applied.

Application for EC type-approval
Article 2
1
The manufacturer or his representative shall submit to the type-approval authority an application drawn up in accordance with the provisions of this Regulation.
2
An application for EC type-approval following one or more of the procedures of Article 1(2) of this Regulation shall consist of the information folder containing the particulars required by the measures implementing Regulation (EC) No 661/2009 setting out requirements in areas covered by UNECE regulations, and shall be made in accordance with Annex I to Directive 2007/46/EC.
3
The type-approval authority shall confirm that it considers the application to be complete.
4
Any EC or UNECE type-approved components and separate technical units which are installed on a vehicle or incorporated within a second component or separate technical unit need not to be fully described in terms of their particulars in the information document if the type-approval numbers and markings are provided in the information document and the relevant type-approval certificates with annexed information packages are made available to the technical service.
5
Components and separate technical units which have a valid EC type-approval mark shall be accepted even in cases where they are applied instead of components and separate technical units that are required to bear an ECE type-approval mark in the context of measures implementing Regulation (EC) No 661/2009 setting out requirements in areas covered by UNECE regulations.

Type-approval
Article 3
1
Where the type of vehicle, component or separate technical unit presented for type-approval complies with the relevant technical prescriptions and measures to ensure conformity of production with the UNECE regulations made compulsory by Regulation (EC) No 661/2009 and where the applicant fulfils the relevant requirements laid down in Article 2 of this Regulation, the type-approval authority shall grant an EC type-approval pursuant to Article 13(15)(a) of Regulation (EC) No 661/2009 and issue a type-approval number in accordance with the numbering system set out in Annex VII to Directive 2007/46/EC.
2
A Member State may not assign the same number to another type of vehicle, component or separate technical unit.
3
For the purposes of paragraph 1, the type-approval authority shall deliver an EC type-approval certificate established in accordance with the model set out in Part 2 of Annex I in case of a type of vehicle, component or separate technical unit incorporating new technologies or new concepts incompatible with UNECE regulations, or Part 3 of Annex I in case of a type of vehicle, component or separate technical unit complying with the essential technical requirements of UNECE regulations and/or in case of self-testing and/or virtual testing.

New technologies or new concepts incompatible with the acts implementing Regulation (EC) No 661/2009 covered by UNECE regulations
Article 4
1
Where a Member State is authorised to grant EC type-approval of a vehicle with regard to a system, component or separate technical unit, in accordance with Article 20 of Directive 2007/46/EC, the procedure set out in paragraphs 2 to 5 shall be followed.
2
The type-approval authority shall grant an EC type-approval pursuant to Article 3 of this Regulation and issue a type-approval number in accordance with the numbering system set out in Annex VII to Directive 2007/46/EC.
3
The type-approval authority shall deliver an EC type-approval certificate established in accordance with the model set out in Part 2 of Annex I with annexed thereto the completed communication form conforming to the relevant model in the applied UNECE regulation with the entry of its UNECE type-approval number left blank.
4
The information folder in accordance with Article 2 shall subsequently be annexed to the type-approval certificate and communication form referred to in paragraph 3 of this Article.
5
Where applicable, an example of the EC type-approval marking, in accordance with the Appendix to Annex VII to Directive 2007/46/EC, shall be provided in the type-approval certificate referred to in paragraph 3 of this Article.

Self-testing
Article 5
1
In line with Articles 11(1) and 41(6) of Directive 2007/46/EC and Annexes V and XV thereto, a manufacturer may be appointed as technical service. The general conditions which the designation of a manufacturer as a technical service shall fulfil are set out in the Appendix to Annex XV to Directive 2007/46/EC. The prescriptions as amended by this Regulation shall apply and the procedure set out in paragraphs 2 to 5 shall be followed.
2
The type-approval authority shall grant an EC type-approval pursuant to Article 3 of this Regulation and issue a type-approval number in accordance with the numbering system set out in Annex VII to Directive 2007/46/EC.
3
The type-approval authority shall deliver an EC type-approval certificate established in accordance with the model set out in Part 3 of Annex I with annexed thereto the completed communication form conforming to the relevant model in the applied UNECE regulation with the entry of its UNECE type-approval number left blank.
4
The information folder in accordance with Article 2 shall subsequently be annexed to the type-approval certificate and communication form referred to in paragraph 3 of this Article.
5
Where applicable, an example of the EC type-approval marking, in accordance with the Appendix to Annex VII to Directive 2007/46/EC, shall be provided in the type-approval certificate referred to in paragraph 3 of this Article.

Virtual testing
Article 6
1
In line with Article 11(4) of Directive 2007/46/EC and Annex XVI thereto, virtual testing methods are permitted, provided that the prescriptions set out in the Appendices to Annex XVI to Directive 2007/46/EC are fulfilled. The prescriptions as amended by this Regulation shall apply and the procedure set out in paragraphs 2 to 5 shall be followed.
2
The type-approval authority shall grant an EC type-approval pursuant to Article 3 of this Regulation and issue a type-approval number in accordance with the numbering system set out in Annex VII to Directive 2007/46/EC.
3
The type-approval authority shall deliver an EC type-approval certificate established in accordance with the model set out in Part 3 of Annex I with annexed thereto the completed communication form conforming to the relevant model in the applied UNECE regulation with the entry of its UNECE type-approval number left blank.
4
The information folder in accordance with Article 2 shall subsequently be annexed to the type-approval certificate and communication form referred to in paragraph 3 of this Article.
5
Where applicable, an example of the EC type-approval marking, in accordance with the Appendix to Annex VII to Directive 2007/46/EC, shall be provided in the type-approval certificate referred to in paragraph 3 of this Article.

Replacement brake lining assemblies, replacement brake discs and replacement brake drums
Article 7
1
With effect from 1 November 2014, UNECE Regulation No 90 shall apply for the purposes of the sale and entry into service of new replacement brake lining assemblies concerning vehicle types of categories M1 with a permissible maximum laden mass not exceeding 3,5 tonnes, M2 with a permissible maximum laden mass not exceeding 3,5 tonnes, N1, O1 and O 2, for which vehicle type-approval is granted in accordance with Directive 71/320/EEC, UNECE Regulation No 13 or UNECE Regulation No 13-H on or after 7 April 1998.
2
With effect from 1 November 2014, UNECE Regulation No 90 shall apply for the purposes of the sale and entry into service of new replacement brake lining assemblies concerning vehicle types of categories M1 with a permissible maximum laden mass exceeding 3,5 tonnes, M2 with a permissible maximum laden mass exceeding 3,5 tonnes, M3, N2, N3, O3 and O 4, for which vehicle type-approval is granted in accordance with UNECE Regulation No 13 or UNECE Regulation No 13-H on or after 1 November 2014.
3
With effect from 1 November 2016, UNECE Regulation No 90 shall apply for the purposes of the sale and entry into service of new replacement brake discs and drums concerning vehicle types of categories M1 and N1 for which vehicle type-approval is granted in accordance with UNECE Regulation No 13 or UNECE Regulation No 13-H on or after 1 November 2016.
4
With effect from 1 November 2014, UNECE Regulation No 90 shall apply for the purposes of the sale and entry into service of new replacement brake discs concerning vehicle types of categories M2, M3, N2 and N 3, for which vehicle type-approval is granted in accordance with UNECE Regulation No 13 on or after 1 November 2014.
5
With effect from 1 November 2016, UNECE Regulation No 90 shall apply for the purposes of the sale and entry into service of new replacement brake drums concerning vehicle types of categories M2, M3, N2 and N 3, for which vehicle type-approval is granted in accordance with UNECE Regulation No 13 on or after 1 November 2016.
6
With effect from 1 November 2016, UNECE Regulation No 90 shall apply for the purposes of the sale and entry into service of new replacement brake discs and drums concerning vehicle types of categories O1 and O2 for which vehicle type-approval is granted in accordance with UNECE Regulation No 13 on or after 1 November 2016.
7
With effect from 1 November 2014, UNECE Regulation No 90 shall apply for the purposes of the sale and entry into service of new replacement brake discs concerning vehicle types of categories O3 and O4 for which vehicle type-approval is granted in accordance with UNECE Regulation No 13 on or after 1 November 2014.
8
With effect from 1 November 2016, UNECE Regulation No 90 shall apply for the purposes of the sale and entry into service of new replacement brake drums concerning vehicle types of categories O3 and O4 for which vehicle type-approval is granted in accordance with UNECE Regulation No 13 on or after 1 November 2016.

Commercial vehicle cab strength
Article 8
1
With effect from 30 January 2017, national authorities shall refuse, on grounds relating to the protection of the occupants of the cab of a commercial vehicle, to grant EC type-approval or national type-approval in respect of new types of vehicle of category N which do not comply with the provisions of UNECE Regulation No 29.
2
With effect from 30 January 2021, national authorities shall, on grounds relating to the protection of the occupants of the cab of a commercial vehicle, consider the certificates of conformity to be no longer valid for the purposes of Article 26 of Directive 2007/46/EC, and shall prohibit the registration, sale and entry into service of vehicles of category N which do not comply with the provisions of UNECE Regulation No 29.

Amendments to Regulation (EC) No 661/2009
Article 9
1
Annex I to Regulation (EC) No 661/2009 is amended in accordance with Annex II to this Regulation.
2
Annex IV to Regulation (EC) No 661/2009 is replaced by the text in Annex III to this Regulation.

Amendments to Directive 2007/46/EC
Article 10
Annexes I, IV, VII, XI, XV and XVI to Directive 2007/46/EC are amended in accordance with Annex IV to this Regulation.

Amendments to Regulation (EU) No 1003/2010
Article 11
Annex II to Regulation (EU) No 1003/2010 is amended in accordance with Annex V to this Regulation.

Amendments to Regulation (EU) No 109/2011
Article 12
1
Article 1 is replaced by the following:

Scope
Article 1
This Regulation applies to vehicles of categories N and O, as defined in Annex II to Directive 2007/46/EC, as well as to spray suppression systems intended for fitment to vehicles of categories N and O.
.
2
Annexes I and IV to Regulation (EU) No 109/2011 are amended in accordance with Annex VI to this Regulation.

Amendments to Regulation (EU) No 458/2011
Article 13
Annex I to Regulation (EU) No 458/2011 is amended in accordance with Annex VII to this Regulation.

Entry into force
Article 14
This Regulation shall enter into force on the twentieth day following that of its publication in the Official Journal of the European Union.
This Regulation shall be binding in its entirety and directly applicable in all Member States.
Done at Brussels, 3 February 2015.
For the Commission
The President
Jean-Claude Juncker
ANNEX I

Administrative provisions for the type-approval of vehicles, components or separate technical units for measures implementing Regulation (EC) No 661/2009 setting out requirements in areas covered by UNECE regulations
PART 1

Information document

MODEL
Information document No … relating to the EC type-approval of a vehicle with regard to a system/component/separate technical unit with regard to UNECE Regulation No … concerning … based on and formatted according to the item numbering of Annex I to Directive 2007/46/EC
The following information, where applicable, shall be supplied in triplicate and include a list of contents. Any drawings shall be supplied in appropriate scale and in sufficient detail on size A4 or on a folder of A4 format. Photographs, if any, shall show sufficient detail.
Where the systems, components or separate technical units referred to in this information document have electronic controls, information concerning their performance shall be supplied.
0.

GENERAL
0.1.
Make (trade name of manufacturer):
0.2.
Type:
0.2.1.
Commercial name(s) (if available):
0.3.
Means of identification of type, if marked on the vehicle/component/separate technical unit :
0.3.1.
Location of that marking:
0.4.
Category of vehicle :
0.5.
Company name and address of manufacturer:
0.8.
Name(s) and address(es) of assembly plant(s):
0.9.
Name and address of the manufacturer's representative (if any)
1.

GENERAL CONSTRUCTION CHARACTERISTICS
1.1.
Photographs and/or drawings of a representative vehicle/component/separate technical unit :
All subsequent items and information relevant for the vehicle, component or separate technical unit shall be provided in agreement with the technical service and type-approval authority responsible for granting the EC type-approval for which the application was submitted. It may be based on a model for an information document if provided by UNECE Regulation No …, otherwise it shall insofar practicable be based on the item numbering of Annex I to Directive 2007/46/EC (i.e. the complete list of information for the purpose of EC type-approval of vehicles, components and separate technical units) and any additional information or particulars required for approval under UNECE Regulation No … shall be included.

Explanatory notes:
PART 2

EC type-approval certificate
MODEL

Format: A4 (210 × 297 mm)
EC TYPE-APPROVAL CERTIFICATE

(IN ACCORDANCE WITH ARTICLE 20 OF THE FRAMEWORK DIRECTIVE)
Stamp of type-approval authority
Communication concerning:
Delete where not applicable.
- EC type-approval - extension of EC type-approval - refusal of EC type-approval - withdrawal of EC type-approval | of a type of vehicle with regard to a system/component/separate technical unit incorporating new technologies or new concepts incompatible with UNECE Regulation No …
with regard to Regulation (EC) No 661/2009, as last amended by Regulation (EU) …/…
EC type-approval number:
Reason for extension:
SECTION I
0.1.
Make (trade name of manufacturer):
0.2.
Type:
0.2.1.
Commercial name(s) (if available):
0.3.
Means of identification of type, if marked on the vehicle/component/separate technical unit :
0.3.1.
Location of that marking:
0.4.
Category of vehicle :
0.5.
Name and address of manufacturer:
0.8.
Name(s) and address(es) of assembly plant(s):
0.9.
Name and address of the manufacturer's representative (if any):
SECTION II
1.
Additional information: see Addendum.
2.
Technical service responsible for carrying out the tests:
3.
Date of test report:
4.
Number of test report:
5.
Remarks (if any): see Addendum.
6.
Place:
7.
Date:
8.
Signature:
Attachments:
- Information package
- Test report
- Completed communication form conforming to the relevant model in the applicable UNECE Regulation, albeit without the mentioning of an UNECE approval being granted or extended as well as without the mentioning of an UNECE type-approval number.
NB: If this model is used for type-approval pursuant to Article 20 of Directive 2007/46/EC it shall not bear the heading ‘EC Vehicle Type-Approval Certificate’, except in the case mentioned in Article 20 where the Commission has decided to allow a Member State to grant a type-approval in accordance with the Framework Directive.
Addendum

to EC type-approval certificate No …
1.
Approval procedure according to Article 20 of Directive 2007/46/EC (exemptions for new technologies or new concepts), authorised by the Commission: yes/no
2.
Implementing measure of Regulation (EC) No 661/2009 forming the basis of this EC type-approval: UNECE Regulation No … concerning
3.
In case of components and separate technical units, example of the type-approval marking on the component or separate technical unit:
4.
EC type-approval valid until (DD/MM/YYYY):
5.
Remarks:
PART 3

EC type-approval certificate
MODEL

Format: A4 (210 × 297 mm)

EC TYPE-APPROVAL CERTIFICATE
Stamp of type-approval authority
Communication concerning:
Delete where not applicable.
- EC type-approval - extension of EC type-approval - refusal of EC type-approval - withdrawal of EC type-approval | of a type of vehicle with regard to a system/component/separate technical unit complying with the requirements laid down in UNECE Regulation No … as amended by supplement … to the … series
with regard to Regulation (EC) No 661/2009, as last amended by Regulation (EU) …/…
EC type-approval number:
Reason for extension:
SECTION I
0.1.
Make (trade name of manufacturer):
0.2.
Type:
0.2.1.
Commercial name(s) (if available):
0.3.
Means of identification of type, if marked on the vehicle/component/separate technical unit :
0.3.1.
Location of that marking:
0.4.
Category of vehicle :
0.5.
Name and address of manufacturer:
0.8.
Name(s) and address(es) of assembly plant(s):
0.9.
Name and address of the manufacturer's representative (if any):
SECTION II
1.
Additional information: see Addendum.
2.
Technical service responsible for carrying out the tests:
3.
Date of test report:
4.
Number of test report:
5.
Remarks (if any): see Addendum.
6.
Place:
7.
Date:
8.
Signature:
Attachments:
- Information package
- Test report
- Completed communication form conforming to the relevant model in the applicable UNECE Regulation, albeit without the mentioning of an UNECE approval being granted or extended as well as without the mentioning of an UNECE type-approval number.
Addendum

to EC type-approval certificate No …
1.
Based on UNECE Regulation using EC type-approved components or separate technical units: yes/no
2.
Approval procedure according to Articles 11(1) and 41(6) of Directive 2007/46/EC (self-testing): yes/no
3.
Approval procedure according to Article 11(4) of Directive 2007/46/EC (virtual testing): yes/no
4.
In case of components and separate technical units, example of the type-approval marking on the component or separate technical unit:
5.
Remarks:
ANNEX II

Amendments to scope of application of Regulation (EC) No 661/2009
Annex I to Regulation (EC) No 661/2009 is amended as follows:
1. the row ‘Spray-suppression systems’ is replaced by the following:
Spray-suppression systems | | | | X | X | X | X | X | X | X
2. the following row is added to the end the list:
Electric safety | X | X | X | X | X | X | | | |
ANNEX III

Amendments to Regulation (EC) No 661/2009
ANNEX IV

List of UNECE Regulations which apply on a compulsory basis
Regulation Number | Subject | Series of amendments published in the OJ | OJ Reference | Scope covered by the UNECE Regulation
1 | Headlamps emitting an asymmetrical passing beam and/or driving beam equipped with filament lamps R2 and/or HS1 | 02 series of amendments | OJ L 177, 10.7.2010, p. 1. | M, N (a)
3 | Retro-reflecting devices for power-driven vehicles | Supplement 12 to the 02 series of amendments | OJ L 323, 6.12.2011, p. 1. | M, N, O
4 | Illumination of rear-registration plates of power-driven vehicles and their trailers | Supplement 15 to the original version of the Regulation | OJ L 4, 7.1.2012, p. 7. | M, N, O
6 | Direction indicators for power-driven vehicles and their trailers | Supplement 25 to the 01 series of amendments | OJ L 213, 18.7.2014, p. 1. | M, N, O
7 | Front and rear position (side) lamps, stop-lamps and end-outline marker lamps for power-driven vehicles and their trailers | Supplement 23 to the 02 series of amendments | OJ L 285, 30.9.2014, p. 1. | M, N, O
8 | Motor vehicles headlamps (H1, H2, H3, HB3, HB4, H7, H8, H9, HIR1, HIR2 and/or H11) | 05 series of amendments Corrigendum 1 to Revision 4 | OJ L 177, 10.7.2010, p. 71. | M, N (a)
10 | Electromagnetic compatibility | Supplement 1 to the 04 series of amendments | OJ L 254, 20.9.2012, p. 1. | M, N, O
11 | Door latches and door retention components | Supplement 2 to the 03 series of amendments | OJ L 120, 13.5.2010, p. 1. | M1, N1
12 | Protection of the driver against the steering mechanism in the event of impact | Supplement 1 to the 04 series of amendments | OJ L 89, 27.3.2013, p. 1. | M1, N1
13 | Braking of vehicles and trailers | Supplement 3 to the 11 series of amendments | OJ L 297, 13.11.2010, p. 183. | M2, M3, N, O (b)
13-H | Braking of passenger cars | Supplement 9 to the original version of the Regulation | OJ L 230, 31.8.2010, p. 1. | M1, N1 (c)
14 | Safety-belt anchorages, ISOFIX anchorages systems and ISOFIX top tether anchorages | Supplement 1 to the 07 series of amendments | OJ L 109, 28.4.2011, p. 1. | M, N
16 | Safety-belts, restraint systems, child restraint systems and ISOFIX child restraint systems | Supplement 1 to the 06 series of amendments | OJ L 233, 9.9.2011, p. 1. | M, N (d)
17 | Seats, their anchorages and any head restraints | 08 series of amendments | OJ L 230, 31.8.2010, p. 81. | M, N
18 | Protection of motor vehicles against unauthorized use | Supplement 2 to the 03 series of amendments | OJ L 120, 13.5.2010, p. 29. | M2, M3, N2, N3
19 | Power-driven vehicle front fog lamps | Supplement 6 to the 04 series of amendments | OJ L 250, 22.8.2014, p. 1. | M, N
20 | Headlamps emitting an asymmetrical passing beam or a driving beam or both and equipped with halogen filament lamps (H4) | 03 series of amendments | OJ L 177, 10.7.2010, p. 170. | M, N (a)
21 | Interior fittings | Supplement 3 to the 01 series of amendments | OJ L 188, 16.7.2008, p. 32. | M1
23 | Reversing lights for power-driven vehicles and their trailers | Supplement 19 to the original version of the Regulation | OJ L 237, 8.8.2014, p. 1. | M, N, O
25 | Head restraints (headrests), whether or not incorporated in vehicle seats | 04 series of amendments Corrigendum 2 to Revision 1 | OJ L 215, 14.8.2010, p. 1. | M1
26 | External projections | Supplement 1 to the 03 series of amendments | OJ L 215, 14.8.2010, p. 27. | M1
28 | Audible warning devices and signals | Supplement 3 to the original version of the Regulation | OJ L 323, 6.12.2011, p. 33. | M, N
29 | Protection of the occupants of the cab of a commercial vehicle | 03 series of amendments | OJ L 304, 20.11.2010, p. 21. | N
30 | Pneumatic tyres for motor vehicles and their trailers (Class C1) | Supplement 16 to the 02 series of amendments | OJ L 307, 23.11.2011, p. 1. | M, N, O
31 | Power-driven vehicle's sealed-beam headlamps (SB) emitting an European asymmetrical passing beam or a driving beam or both | Supplement 7 to the 02 series of amendments | OJ L 185, 17.7.2010, p. 15. | M, N
34 | Prevention of fire risks (liquid fuel tanks) | Supplement 3 to the 02 series of amendments | OJ L 109, 28.4.2011, p. 55. | M, N, O (e)
37 | Filament lamps for use in approved lamp units of power-driven vehicles and their trailers | Supplement 42 to the 03 series of amendments | OJ L 213, 18.7.2014, p. 36. | M, N, O
38 | Rear fog lamps for power-driven vehicles and their trailers | Supplement 15 to the original version of the Regulation | OJ L 4, 7.1.2012, p. 20. | M, N, O
39 | Speedometer equipment including its installation | Supplement 5 to the original version of the Regulation | OJ L 120, 13.5.2010, p. 40. | M, N
43 | Safety glazing materials | Supplement 2 to the 01 series of amendments | OJ L 42, 12.2.2014, p. 1. | M, N, O
44 | Restraining devices for child occupants of power-driven vehicles (“child restraint system”) | Corrigendum 4 to Revision 2 of the 04 series of amendments | OJ L 233, 9.9.2011, p. 95. | M, N
46 | Devices for indirect vision and their installation | Supplement 1 to the 04 series of amendments | OJ L 237, 8.8.2014, p. 24. | M, N
48 | Installation of lighting and light-signalling devices on motor vehicles | 05 series of amendments | OJ L 323, 6.12.2011, p. 46. | M, N, O
54 | Pneumatic tyres for commercial vehicles and their trailers (Classes C2 and C3) | Supplement 17 to the original version of the Regulation | OJ L 307, 23.11.2011, p. 2. | M, N, O
55 | Mechanical coupling components of combinations of vehicles | Supplement 1 to the 01 series of amendments | OJ L 227, 28.8.2010, p. 1. | M, N, O (f)
58 | Rear underrun protective devices (RUPDs) and their installation; Rear underrun protection (RUP) | Supplement 3 to the 02 series of amendments | OJ L 89, 27.3.2013, p. 34. | N2, N3, O3, O4
61 | Commercial vehicles with regard to their external projections forward of the cab's rear panel | Supplement 1 to the original version of the Regulation | OJ L 164, 30.6.2010, p. 1. | N
64 | Temporary-use spare unit, run-flat tyres/system and tyre pressure monitoring system | Corrigendum 1 to the 02 series of amendments | OJ L 310, 26.11.2010, p. 18. | M1, N1
66 | Strength of the superstructure of large passenger vehicles | 02 series of amendments | OJ L 84, 30.3.2011, p. 1. | M2, M3
67 | Motor vehicles using LPG | Supplement 7 to the 01 series of amendments | OJ L 72, 14.3.2008, p. 1. | M, N
73 | Lateral protection of goods vehicles | 01 series of amendments | OJ L 122, 8.5.2012, p. 1. | N2, N3, O3, O4
77 | Parking lamps for power-driven vehicles | Supplement 14 to the original version of the Regulation | OJ L 4, 7.1.2012, p. 21. | M, N
79 | Steering equipment | Supplement 3 to the 01 series of amendments Corrigendum | OJ L 137, 27.5.2008, p. 25. | M, N, O
80 | Seats of large passenger vehicles | 03 series of amendments to the Regulation | OJ L 226, 24.8.2013, p. 20. | M2, M3
87 | Daytime running lamps for power-driven vehicles | Supplement 15 to the original version of the Regulation | OJ L 4, 7.1.2012, p. 24. | M, N
89 | Speed limitation devices | Supplement 2 to the original version of the Regulation | OJ L 4, 7.1.2012, p. 25. | M, N (g)
90 | Replacement brake lining assemblies and drum brake linings for power-driven vehicles and their trailers | 02 series of amendments | OJ L 185, 13.7.2012, p. 24. | M, N, O
91 | Side-marker lamps for motor vehicles and their trailers | Supplement 13 to the original version of the Regulation | OJ L 4, 7.1.2012, p. 27. | M, N, O
93 | Front underrun protective devices (FUPDs) and their installation; front underrun protection (FUP) | Original version of the Regulation | OJ L 185, 17.7.2010, p. 56. | N2, N3
94 | Protection of occupants in the event of a frontal collision | Supplement 2 to the 02 series of amendments | OJ L 254, 20.9.2012, p. 77. | M1
95 | Protection of occupants in the event of a lateral collision | Supplement 1 to the 02 series of amendments Corrigendum | OJ L 313, 30.11.2007, p. 1. | M1, N1
97 | Vehicle Alarm Systems (VAS) | Supplement 6 to the 01 series of amendments | OJ L 122, 8.5.2012, p. 19. | M1, N1
98 | Motor vehicle headlamps equipped with gas-discharge light sources | Supplement 4 to the 01 series of amendments | OJ L 176, 14.6.2014, p. 64. | M, N
99 | Gas-discharge light sources for use in approved gas-discharge lamp units of power-driven vehicles | Supplement 9 to the original version of the Regulation | OJ L 285, 30.9.2014, p. 35. | M, N
100 | Electric safety | 01 series of amendments | OJ L 57, 2.3.2011, p. 54. | M, N
102 | Close-coupling device (CCD); fitting of an approved type of CCD | Original version of the Regulation | OJ L 351, 30.12.2008, p. 44. | N2, N3, O3, O4
104 | Retro-reflective markings (heavy and long vehicles) | Supplement 7 to the original version | OJ L 75, 14.3.2014, p. 29. | M2, M3, N, O2, O3, O4
105 | Vehicles for the carriage of dangerous goods | 05 series of amendments | OJ L 4, 7.1.2012, p. 30. | N, O
107 | M2 and M3 vehicles | 03 series of amendments | OJ L 255, 29.9.2010. | M2, M3
110 | Specific components for CNG | Supplement 9 to the original version of the Regulation | OJ L 120, 7.5.2011, p. 1. | M, N
112 | Motor vehicle headlamps emitting an asymmetrical passing beam or a driving beam or both and equipped with filament lamps and/or LED modules | Supplement 4 to the 01 series of amendments | OJ L 250, 22.8.2014, p. 67. | M, N
116 | Protection of motor vehicles against unauthorized use | Supplement 3 to the original version of the Regulation | OJ L 45, 16.2.2012, p. 1. | M1, N1
117 | Tyres with regard to rolling sound emissions, adhesion on wet surfaces and rolling resistance (Classes C1, C2 and C3) | Corrigendum 3 to the 02 series of amendments | OJ L 307, 23.11.2011, p. 3. | M, N, O
118 | Burning behaviour of materials used in the interior construction of certain categories of motor vehicles | Original version of the Regulation | OJ L 177, 10.7.2010, p. 263. | M3
119 | Cornering lamps | Supplement 3 to the 01 series of amendments | OJ L 89, 25.3.2014, p. 101. | M, N
121 | Location and identification of hand controls, tell-tales and indicators | Supplement 3 to the original version of the Regulation | OJ L 177, 10.7.2010, p. 290. | M, N
122 | Heating system of vehicles | Supplement 1 to the original version of the Regulation | OJ L 164, 30.6.2010, p. 231. | M, N, O
123 | Adaptive front-lighting systems (AFS) for motor vehicles | Supplement 4 to the original version of the Regulation | OJ L 222, 24.8.2010, p. 1. | M, N
125 | Forward field of vision | Supplement 2 to the original version of the Regulation | OJ L 200, 31.7.2010, p. 38. | M1
128 | Light Emitting Diode (LED) light sources | Supplement 2 to the original version of the Regulation | OJ L 162, 29.5.2014, p. 43. | M, N, O

Notes to the table:
The transitional provisions of the UNECE regulations listed in this table apply, except where specific alternative dates are provided for in this Regulation. Compliance with prescriptions in accordance with subsequent amendments to those listed in this table shall also be accepted.
The dates specified in the UNECE regulations listed in this table, as regards the obligations of Contracting Parties to the “Revised 1958 Agreement” (Council Decision of 27 November 1997 with a view to accession by the European Community to the Agreement of the United Nations Economic Commission for Europe concerning the adoption of uniform technical prescriptions for wheeled vehicles, equipment and parts which can be fitted to and/or be used on wheeled vehicles and the conditions for reciprocal recognition of approvals granted on the basis of these prescriptions (“Revised 1958 Agreement”) (OJ L 346, 17.12.1997, p. 78).), linked to first registration, entry into service, making available on the market, sale, and any similar provisions, apply on a compulsory basis for the purposes of Articles 26 and 28 of Directive 2007/46/EC except in the case where alternative dates are specified in Regulation (EC) No 661/2009, which should then be taken instead.
In certain instances, a UNECE regulation listed in this table provides in its transitional provisions that as from a specified date, Contracting Parties to the “Revised 1958 Agreement”, applying a certain series of amendments to that UNECE regulation, shall not be obliged to accept or may refuse to accept, for the purpose of national or regional type-approval, a type approved in accordance with a preceding series of amendments, or wording with similar intention and meaning. This shall be construed as a binding provision for national authorities to consider the certificates of conformity to be no longer valid for the purposes of Article 26 of Directive 2007/46/EC, except in the case where alternative dates are specified in Regulation (EC) No 661/2009, which should then be taken instead.
(a)
UNECE Regulation Nos 1, 8 and 20 are not applicable for EC type-approval of new vehicles.
(b)
The fitting of an electronic stability control system is required in accordance with Article 12(1) and (2) of Regulation (EC) No 661/2009. Therefore, the application of Annex 21 to UNECE Regulation No 13 is mandatory for the purposes of EC type-approval of new types of vehicles as well as for registration, sale and entry into service of new vehicles. However, the implementation dates concerning electronic stability control systems mentioned in Article 13(1), (4) and (5) as well as Annex V this Regulation shall apply instead of the dates mentioned in that UNECE Regulation.
(c)
The fitting of an electronic stability control system is required in accordance with Article 12(1) of Regulation (EC) No 661/2009. Therefore, the application of Part A of Annex 9 to UNECE Regulation No 13-H is mandatory for the purposes of EC type-approval of new types of vehicles as well as for registration, sale and entry into service of new vehicles. However, the implementation dates concerning electronic stability control systems mentioned in Article 13(1) and (5) of this Regulation shall apply instead of the dates mentioned in that UNECE Regulation.
(d)
A safety-belt reminder is not required for a driver position equipped with an S-type belt or Harness belt.
(e)
Compliance with Part II of UNECE Regulation No 34 is not compulsory.
(f)
Where it is declared by the vehicle manufacturer that a vehicle is suitable for towing loads (point 2.11.5 of Annex I to Directive 2007/46/EC), no mechanical coupling device fitted to the vehicle shall (partly) obscure any lighting component (e.g. rear fog lamp) or the space for mounting and the fixing of the rear registration plate, unless the installed mechanical coupling device can be removed or repositioned without the use of any tools, including release keys.
(g)
Only Speed Limitation Devices (SLD) and the mandatory installation of SLD on vehicles of category M2, M3, N2 and N3 are concerned.
Appendix

Validity and extension of approvals granted under the Directives repealed by this Regulation
In accordance with Article 13(14) of this Regulation, EC type-approval certificates for vehicles, components and separate technical units issued in accordance with the directives listed below may be used to demonstrate compliance with the relevant UNECE regulations.
Regulation Number | Subject | Corresponding Directive | OJ Reference | Applicability
10 | Electromagnetic compatibility | Directive 72/245/EEC | OJ L 152, 6.7.1972, p. 15. | M, N, O, component, STU (a)
11 | Door latches and door retention components | Directive 70/387/EEC | OJ L 176, 10.8.1970, p. 5. | M1, N1 (b)
12 | Protection of the driver against the steering mechanism in the event of impact | Directive 74/297/EEC | OJ L 165, 20.6.1974, p. 16. | M1, N1 (a)
14 | Safety-belt anchorages, ISOFIX anchorages systems and ISOFIX top tether anchorages | Directive 76/115/EEC | OJ L 24, 30.1.1976, p. 6. | M (c)
18 | Protection of motor vehicles against unauthorized use | Directive 74/61/EEC | OJ L 38, 11.2.1974, p. 22. | M2, M3, N2, N3, component, STU
21 | Interior fittings | Directive 74/60/EEC | OJ L 38, 11.2.1974, p. 2. | M1
26 | External projections | Directive 74/483/EEC | OJ L 266, 2.10.1974, p. 4. | M1, STU (d)
28 | Audible warning devices and signals | Directive 70/388/EEC | OJ L 176, 10.8.1970, p. 12. | M, N, component
30 | Pneumatic tyres for motor vehicles and their trailers (Class C1) | Directive 92/23/EEC | OJ L 129, 14.5.1992, p. 95. | component (e)
34 | Prevention of fire risks (liquid fuel tanks) | Directive 70/221/EEC | OJ L 76, 6.4.1970, p. 23. | M, N, O (f)
39 | Speedometer equipment including its installation | Directive 75/443/EEC | OJ L 196, 26.7.1975, p. 1. | M, N (g)
43 | Safety glazing materials | Directive 92/22/EEC | OJ L 129, 14.5.1992, p. 11. | M, N, O, component
46 | Devices for indirect vision and their installation | Directive 2003/97/EC | OJ L 25, 29.1.2004, p. 1. | M, N, component
48 | Installation of lighting and light-signalling devices on motor vehicles | Directive 76/756/EEC | OJ L 262, 27.9.1976, p. 1. | M, N, O
55 | Mechanical coupling components of combinations of vehicles | Directive 94/20/EC | OJ L 195, 29.7.1994, p. 1. | M, N, O, component
58 | Rear underrun protective devices (RUPDs) and their installation; Rear underrun protection (RUP) | Directive 70/221/EEC | OJ L 76, 6.4.1970, p. 23. | M, N, O, STU
61 | Commercial vehicles with regard to their external projections forward of the cab's rear panel | Directive 92/114/EEC | OJ L 409, 31.12.1992, p. 17. | N
73 | Lateral protection of goods vehicles | Directive 89/297/EEC | OJ L 124, 5.5.1989, p. 1. | N2, N3, O3, O4
79 | Steering equipment | Directive 70/311/EEC | OJ L 133, 18.6.1970, p. 10. | M, N, O (h)
89 | Speed limitation devices | Directive 92/24/EEC | OJ L 129, 14.5.1992, p. 154. | M2, M3, N2, N3, STU
90 | Replacement brake lining assemblies and drum brake linings for power-driven vehicles and their trailers | Directive 71/320/EEC | OJ L 202, 6.9.1971, p. 37. | STU (i)
93 | Front underrun protective devices (FUPDs) and their installation; front underrun protection (FUP) | Directive 2000/40/EC | OJ L 203, 10.8.2000, p. 9. | N2, N3, STU
97 | Vehicle Alarm Systems (VAS) | Directive 74/61/EEC | OJ L 38, 11.2.1974, p. 22. | M1, N1, component, STU
116 | Protection of motor vehicles against unauthorized use | Directive 74/61/EEC | OJ L 38, 11.2.1974, p. 22. | M1, N1, component, STU
118 | Burning behaviour of materials used in the interior construction of certain categories of motor vehicles | Directive 95/28/EC | OJ L 281, 23.11.1995, p. 1. | M3, component
122 | Heating system of vehicles | Directive 2001/56/EC | OJ L 292, 9.11.2001, p. 21. | M, N, O, component
125 | Forward field of vision | Directive 77/649/EEC | OJ L 267, 19.10.1977, p. 1. | M1

Notes to the table:
(a)
Not applicable for vehicle types equipped with electric propulsion.
(b)
Not applicable for vehicle types in case of design changes to and/or the introduction of any back door and/or sliding door.
(c)
Only applicable for special purpose completed vehicles of category M1, excluding motor-caravans, with a permissible maximum laden mass exceeding 2,0 tonnes, as well as for vehicle categories M2 and M 3.
(d)
Not applicable for radio receiving or transmitting aerials considered as separate technical units.
(e)
Only applicable for Class C1 tyres manufactured before, on or after 1 November 2014, to be sold and put into service after 1 November 2014 and being identified by means of the letter code “Z” placed within the tyre size designation.
(f)
Not covering Part II of UNECE Regulation No 34.
(g)
See Article 4 of Regulation (EU) No 130/2012 (Commission Regulation (EU) No 130/2012 of 15 February 2012 concerning type-approval requirements for motor vehicles with regard to vehicle access and manoeuvrability and implementing Regulation (EC) No 661/2009 of the European Parliament and of the Council concerning type-approval requirements for the general safety of motor vehicles, their trailers and systems, components and separate technical units intended therefor (OJ L 43, 16.2.2012, p. 6)).
(h)
Not applicable for vehicle types equipped with steering equipment containing complex electronic control systems.
(i)
Notwithstanding the provisions of Article 7(1) of Regulation (EU) 2015/166 and not applicable for brake discs and drums.
ANNEX IV

Amendments to Directive 2007/46/EC
Directive 2007/46/EC is amended as follows:
1. Annex I is amended as follows:
  1. the title is replaced by the following:

Complete list of information for the purpose of EC type-approval of vehicles, components or separate technical units (a)
;
  2. point 0.3 is replaced by the following:
0.3.
Means of identification of type, if marked on the vehicle/component/separate technical unit (1) (b):
;
  3. points 1 and 1.1 are replaced by the following:
1.

GENERAL CONSTRUCTION CHARACTERISTICS
1.1.
Photographs and/or drawings of a representative vehicle/component/separate technical unit (1):
.
2. Part I of Annex IV is amended as follows:
  1. item 6A is replaced by the following:
6A | Vehicle access and manoeuvrability (steps, running boards and handholds) | Regulation (EC) No 661/2009 Regulation (EU) No 130/2012 | X | | | X | X | X | | | |
  2. item 17A is replaced by the following:
17A | Vehicle access and manoeuvrability (reverse gear) | Regulation (EC) No 661/2009 Regulation (EU) No 130/2012 | X | X | X | X | X | X | | | |
  3. item 71 is added:
71 | Cab strength | Regulation (EC) No 661/2009 UNECE Regulation No 29 | | | | X | X | X | | | |
  4. explanatory note 15 is replaced by the following:
(15)
Compliance with Regulation (EC) No 661/2009 is mandatory, however, type-approval under this single item is not provided for as the item covers the combination of individual items 3A, 3B, 4A, 5A, 6A, 6B, 7A, 8A, 9A, 9B, 10A, 12A, 13A, 13B, 14A, 15A, 15B, 16A, 17A, 17B, 18A, 19A, 20A, 21A, 22A, 22B, 22C, 23A, 24A, 25A, 25B, 25C, 25D, 25E, 25F, 26A, 27A, 28A, 29A, 30A, 31A, 32A, 33A, 34A, 35A, 36A, 37A, 38A, 42A, 43A, 44A, 45A, 46A, 46B, 46C, 46D, 46E, 47A, 48A, 49A, 50A, 50B, 51A, 52A, 52B, 53A, 54A, 56A, 57A and 64 to 71.
;
  5. Appendix 1 to Part I of Annex IV is amended as follows:
    1. in Table 1, item 13A is replaced by the following:
13A | Protection of motor vehicles against unauthorised use | Regulation (EC) No 661/2009 UNECE Regulation No 116 | | A The provisions of paragraph 8.3.1.1.1 of UNECE Regulation No 116 may be applied instead of paragraph 8.3.1.1.2 of that Regulation regardless of the type of powertrain
    2. in Table 1, item 63 is replaced by the following:
63 | General Safety | Regulation (EC) No 661/2009 | | See footnote (15) of the table in Part I of Annex IV with regulatory acts for EC type-approval of vehicles produced in unlimited series
    3. in Table 2, item 13A is replaced by the following:
13A | Protection of motor vehicles against unauthorised use | Regulation (EC) No 661/2009 UNECE Regulation No 116 | | A The provisions of paragraph 8.3.1.1.1 of UNECE Regulation No 116 may be applied instead of paragraph 8.3.1.1.2 of that Regulation regardless of the type of powertrain
    4. in Table 2, item 63 is replaced by the following:
63 | General Safety | Regulation (EC) No 661/2009 | | See footnote (15) of the table in Part I of Annex IV with regulatory acts for EC type-approval of vehicles produced in unlimited series
    5. in Table 2, item 71 is added:
71 | Cab strength | Regulation (EC) No 661/2009 UNECE Regulation No 29 | | C
3. Annex VII is amended as follows:
  1. in Section 2, the following paragraph is added:
In case of EC type-approval for systems, components or separate technical units covered by the implementing measures of Regulation (EC) No 661/2009, the base Regulation reference shall be the Regulation number (i.e. the implementing act) adopted pursuant to Article 14(1)(a) to (e) of Regulation (EC) No 661/2009.
;
  2. section 3 is amended as follows:
    1. the first paragraph is replaced by the following:
The number of the latest amending Directive or Regulation, including implementing acts applicable to the type-approval in accordance with the following indents. However, in case such amending Directive or Regulation or applicable implementing act does not yet exist, the number referred to in Section 2 is repeated in Section 3:
;
    2. the following indent is inserted after the third indent:
—
this means the latest Regulation, containing amendments to implementing measures of Regulation (EC) No 661/2009, with which a system, component or technical unit complies,
;
  3. in point 4.1, the following items are added:
    1. to Commission Regulation (EU) No 1008/2010 (windscreen wiper and washer systems)
e2*1008/2010*1008/2010*00003*00
    2. to Commission Regulation (EU) No 19/2011 as amended by Commission Regulation (EU) No 249/2012 (statutory markings)
e2*19/2011*249/2012*0003*00
  4. point 5 is replaced by the following:
5.

Annex VII does not apply to type-approvals granted in accordance with UNECE Regulations listed in Annex IV, as the relevant numbering system is provided for in the respective UNECE Regulations. However, Annex VII applies to EC type-approvals granted under Regulation (EC) No 661/2009 which are based on UNECE Regulations (i.e. incorporating new technologies, EC type-approved components and STUs, virtual testing and self-testing). In this case, the following numbering system is applied:
    - Section 1: as above
    - Section 2: “661/2009” (i.e. General Safety Regulation)
    - Section 3: First portion is the UNECE Regulation No, followed by “R-”, the second portion is the series of amendments or “00” if it is the original series, followed by “-” and the third portion is the supplement level (with leading zeroes if applicable) or “00” when there is no supplement to the relevant series.
    - Section 4: as above
    - Section 5: as above
Examples:
e1*661/2009*13-HR-10-05*00001*00
(granted by Germany, according to UNECE Regulation No 13-H, 10 series of amendments, supplement level 5, first approval issued, no extensions)
e25*661/2009*28R-00-03*0123*05
(granted by Croatia, according to UNECE Regulation No 28, original series of amendments, supplement 3, 123 rd approval issued, 5 th extension)
  5. in the Appendix, point 4 is added:
4.

This Appendix does not apply to type-approvals granted in accordance with UNECE Regulations listed in Annex IV, as the relevant arrangements of approval marks are provided for in the respective UNECE Regulations. However, this Appendix applies to EC component and separate technical unit type-approvals granted under Regulation (EC) No 661/2009 which are based on UNECE Regulations (i.e. components or separate technical units incorporating new technologies). In this case, the following arrangement of markings is applied:
The distinguishing type-approval marking shall be as prescribed in the relevant UNECE Regulation and as if granted through conventional UNECE Regulation type-approval, however, the following shall be taken into account:
When a circle surrounding the letter “E” is prescribed, this shall be not a circle, but a rectangle. Its height (a) shall at least correspond to the prescribed diameter size and its width shall exceed that value (i.e. > a). Instead of the upper-case letter “E”, the lower-case letter “e” shall be used, followed by the distinguishing number of the Member State which has granted the EC component or separate technical unit type-approval.
Example:
(granted by Germany, based on UNECE Regulation No 28, original series, first approval issued, for a Class II audible warning device incorporating new technologies)
4. Annex XI is amended as follows:
  1. in Appendix 3, item 1A is replaced by the following:
1A | Sound level | Regulation (EU) No 540/2014 | G + W9
  2. in Appendix 5, item 1A is replaced by the following:
1A | Sound level | Regulation (EU) No 540/2014 | T + Z1
  3. in Appendix 6, meaning of notes, the following note is inserted after W8:
W9
Modification of the exhaust system length is permitted without the need for retesting, provided that the exhaust back pressure characteristics remain similar.
5. In Annex XV, point 2 is replaced by the following:
2.

List of regulatory acts and restrictions
| Subject | Regulatory act reference
4 | Rear registration plate space | Directive 70/222/EEC
4A | Space for mounting and fixing rear registration plates | Regulation (EC) No 661/2009 Regulation (EU) No 1003/2010
7 | Audible warning | Directive 70/388/EEC
7A | Audible warning devices and signals | Regulation (EC) No 661/2009 UNECE Regulation No 28
10 | Radio interference (electromagnetic compatibility) | Directive 72/245/EEC
10A | Electromagnetic compatibility | Regulation (EC) No 661/2009 UNECE Regulation No 10
18 | Plates (statutory) | Directive 76/114/EEC
18A | Manufacturer's statutory plate and vehicle identification number | Regulation (EC) No 661/2009 Regulation (EU) No 19/2011
20 | Installation of lighting and light signalling devices | Directive 76/756/EEC
20A | Installation of lighting and light-signalling devices on vehicles | Regulation (EC) No 661/2009 UNECE Regulation No 48
27 | Towing hooks | Directive 77/389/EEC
27A | Towing device | Regulation (EC) No 661/2009 Regulation (EU) No 1005/2010
33 | Identification of controls, tell-tales and indicators | Directive 78/316/EEC
33A | Location and identification of hand controls, tell-tales and indicators | Regulation (EC) No 661/2009 UNECE Regulation No 121
34 | Defrost/demist | Directive 78/317/EEC
34A | Windscreen defrosting and demisting systems | Regulation (EC) No 661/2009 Regulation (EU) No 672/2010
35 | Wash/wipe | Directive 78/318/EEC
35A | Windscreen wiper and washer systems | Regulation (EC) No 661/2009 Regulation (EU) No 1008/2010
36 | Heating systems | Directive 2001/56/EC Except the provisions in Annex VIII relating to LPG combustion heaters and LPG heating systems
36A | Heating systems | Regulation (EC) No 661/2009 UNECE Regulation No 122 Except the provisions in Annex 8 relating to LPG combustion heaters and LPG heating systems
37 | Wheel guards | Directive 78/549/EEC
37A | Wheel guards | Regulation (EC) No 661/2009 Regulation (EU) No 1009/2010
44 | Masses and dimensions (cars) | Directive 92/21/EEC
44A | Masses and dimensions | Regulation (EC) No 661/2009 Regulation (EU) No 1230/2012
45 | Safety glazing | Directive 92/22/EEC Restricted to the provisions included in Annex III
45A | Safety glazing materials and their installation on vehicles | Regulation (EC) No 661/2009 UNECE Regulation No 43 Restricted to the provisions included in Annex 21
46 | Tyres | Directive 92/23/EEC
46A | Installation of tyres | Regulation (EC) No 661/2009 Regulation (EU) No 458/2011
48 | Masses and dimensions (other than vehicles referred to in item 44) | Directive 97/27/EC
48A | Masses and dimensions | Regulation (EC) No 661/2009 Regulation (EU) No 1230/2012
49 | External projections of cabs | Directive 92/114/EEC
49A | Commercial vehicles with regard to their external projections forward of the cab's rear panel | Regulation (EC) No 661/2009 UNECE Regulation No 61
50 | Couplings | Directive 94/20/EC Restricted to the provisions included in Annex V (up to and including point 8) and Annex VII
50A | Mechanical coupling components of combinations of vehicles | Regulation (EC) No 661/2009 UNECE Regulation No 55 Restricted to the provisions included in Annex 5 (up to and including paragraph 8) and Annex 7
61 | Air-conditioning system | Directive 2006/40/EC
6. Annex XVI is amended as follows:
  1. point 1 is replaced by the following:
1.

List of regulatory acts
| Subject | Regulatory act reference
3 | Fuel tanks/rear protective devices | Directive 70/221/EEC
3B | Rear underrun protective devices (RUPDs) and their installation; rear underrun protection (RUP) | Regulation (EC) No 661/2009 UNECE Regulation No 58
6 | Door latches and hinges | Directive 70/387/EEC
6A | Vehicle access and manoeuvrability | Regulation (EC) No 661/2009 Regulation (EU) No 130/2012
6B | Door latches and door retention components | Regulation (EC) No 661/2009 UNECE Regulation No 11
8 | Indirect vision devices | Directive 2003/97/EC
8A | Devices for indirect vision and their installation | Regulation (EC) No 661/2009 UNECE Regulation No 46
12 | Interior fittings | Directive 74/60/EEC
12A | Interior fittings | Regulation (EC) No 661/2009 UNECE Regulation No 21
16 | Exterior projections | Directive 74/483/EEC
16A | External projections | Regulation (EC) No 661/2009 UNECE Regulation No 26
20 | Installation of lighting and light signalling devices | Directive 76/756/EEC
20A | Installation of lighting and light-signalling devices on vehicles | Regulation (EC) No 661/2009 UNECE Regulation No 48
27 | Towing hooks | Directive 77/389/EEC
27A | Towing device | Regulation (EC) No 661/2009 Regulation (EU) No 1005/2010
32 | Forward vision | Directive 77/649/EEC
32A | Forward field of vision | Regulation (EC) No 661/2009 UNECE Regulation No 125
35 | Wash/wipe | Directive 78/318/EEC
35A | Windscreen wiper and washer systems | Regulation (EC) No 661/2009 Regulation (EU) No 1008/2010
37 | Wheel guards | Directive 78/549/EEC
37A | Wheel guards | Regulation (EC) No 661/2009 Regulation (EU) No 1009/2010
42 | Lateral protection | Directive 89/297/EEC
42A | Lateral protection of goods vehicles | Regulation (EC) No 661/2009 UNECE Regulation No 73
48A | Masses and dimensions | Regulation (EC) No 661/2009 Regulation (EU) No 1230/2012
49 | External projections of cabs | Directive 92/114/EEC
49A | Commercial vehicles with regard to their external projections forward of the cab's rear panel | Regulation (EC) No 661/2009 UNECE Regulation No 61
50 | Couplings | Directive 94/20/EC
50A | Mechanical coupling components of combinations of vehicles | Regulation (EC) No 661/2009 UNECE Regulation No 55
50B | Close-coupling device (CCD); fitting of an approved type of CCD | Regulation (EC) No 661/2009 UNECE Regulation No 102
52 | Buses and coaches | Directive 2001/85/EC
52A | M2 and M3 vehicles | Regulation (EC) No 661/2009 UNECE Regulation No 107
52B | Strength of the superstructure of large passenger vehicles | Regulation (EC) No 661/2009 UNECE Regulation No 66
57 | Front underrun protection | Directive 2000/40/EC
57A | Front underrun protective devices (FUPDs) and their installation; front underrun protection (FUP) | Regulation (EC) No 661/2009 UNECE Regulation No 93
  2. Appendix 2 is replaced by the following:
Appendix 2

Specific conditions concerning virtual testing methods
1.

List of regulatory acts
| Regulatory act reference | Annex and paragraphs | Specific conditions
3 | Directive 70/221/EEC | Annex II, points 5.2 and 5.4.5 | Rear underrun dimensions and resistance to forces
3B | Regulation (EC) No 661/2009 UNECE Regulation No 58 | Paragraphs 2.3, 7.3 and 25.6 | Dimensions and resistance to forces
6 | Directive 70/387/EEC | Annex II, point 4.3 | Equivalent methods for tensile strength tests and resistance of latches to acceleration
6A | Regulation (EC) No 661/2009 Regulation (EU) No 130/2012 | Annex II, Part I and 2 | Dimensions of steps, running boards and handholds
6B | Regulation (EC) No 661/2009 UNECE Regulation No 11 | Annex 3 Annex 4, point 2.1 Annex 5 | Tensile strength tests and resistance of latches to acceleration
8 | Directive 2003/97/EC | Annex III All provisions in Sections 3, 4 and 5. | Prescribed fields of vision of rear-view mirrors.
8A | Regulation (EC) No 661/2009 UNECE Regulation No 46 | Paragraph 15.2.4 | Prescribed fields of vision of rear-view mirrors.
12 | Directive 74/60/EEC | 1. Annex I, all provisions in point 5 (Specifications) 2. Annex II | 1. Measurement of all radii of curvature and of all projections except for those requirements where a force has to be applied in order to check compliance with the provisions. 2. Determination of the head-impact zone.
12A | Regulation (EC) No 661/2009 UNECE Regulation No 21 | 1. Paragraph 5 to 5.7 2. Paragraph 2.3 | 1. Measurement of all radii of curvature and of all projections except for those requirements where a force has to be applied in order to check compliance with the provisions. 2. Determination of the head-impact zone.
16 | Directive 74/483/EEC | Annex I, all provisions in point 5 (General specifications) and point 6 (Particular specifications). | Measurement of all radii of curvature and of all projections except for those requirements where a force has to be applied in order to check compliance with the provisions.
16A | Regulation (EC) No 661/2009 UNECE Regulation No 26 | Paragraph 5.2.4 | Measurement of all radii of curvature and of all projections except for those requirements where a force has to be applied in order to check compliance with the provisions.
20 | Directive 76/756/EEC | Paragraph 6 (Individual specifications) of UNECE Regulation No 48. Provisions of Annexes 4, 5 and 6 to UNECE Regulation No 48. | The test drive provided for in point 6.22.9.2.2 shall be performed on a real vehicle.
20A. | Regulation (EC) No 661/2009 UNECE Regulation No 48 | Paragraph 6, Annexes 4, 5 and 6 | The test drive provided for in point 6.22.9.2.2 shall be performed on a real vehicle.
27 | Directive 77/389/EEC | Annex II, point 2 | Tractive and compressive static force
27A | Regulation (EC) No 661/2009 Regulation (EU) No 1005/2010 | Annex II, point 1.2 | Tractive and compressive static force
32 | Directive 77/649/EEC | Annex I, point 5 (Specifications) | Obstructions and field of vision
32A | Regulation (EC) No 661/2009 UNECE Regulation No 125 | Paragraph 5 | Obstructions and field of vision
35 | Directive 78/318/EEC | Annex I, point 5.1.2 | Determination of the swept area only.
35A | Regulation (EC) No 661/2009 Regulation (EU) No 1008/2010 | Annex III, points 1.1.2 and 1.1.3 | Determination of the swept area only.
37 | Directive 78/549/EEC | Annex I, point 2 (Special requirements) |
37A | Regulation (EC) No 661/2009 Regulation (EU) No 1009/2010 | Annex II, point 2 | Verification of the dimensional requirements
42 | Directive 89/297/EEC | Annex, point 2.8 | Resistance under a horizontal force and deflection measurement.
42A | Regulation (EC) No 661/2009 UNECE Regulation No 73 | Paragraph 12.10 | Resistance under a horizontal force and deflection measurement.
48A. | Regulation (EC) No 661/2009 Regulation (EU) No 1230/2012 | 1. Annex I, Part B, points 7 and 8 2. Annex I, Part C, points 6 and 7 | 1. Check of compliance with the manoeuvrability requirements including manoeuvrability of vehicles fitted with lift- or loadable axles. 2. Measurement of the maximum rear swing-out.
49 | Directive 92/114/EEC | Annex I, point 4 (Specific requirements) | Measurement of all radii of curvature and of all projections except for those requirements where a force has to be applied in order to check compliance with the provisions.
49A | Regulation (EC) No 661/2009 UNECE Regulation No 61 | Paragraphs 5 and 6 | Measurement of all radii of curvature and of all projections except for those requirements where a force has to be applied in order to check compliance with the provisions.
50 | Directive 94/20/EC | 1. Annex V “Requirements for mechanical coupling Devices” 2. Annex VI, point 1.1 3. Annex VI, point 4 (Testing of mechanical coupling devices) | 1. All provisions of points 1 to 8 included. 2. Strength tests on mechanicals couplings of simple design may be replaced by virtual tests. 3. Points 4.5.1 (Strength test), 4.5.2 (Resistance to buckling) and 4.5.3 (Resistance to bending moment) only.
50A | Regulation (EC) No 661/2009 UNECE Regulation No 55 | 1. Annex 5 “Requirements for mechanical coupling Devices” 2. Annex 6, paragraph 1.1 3. Annex 6, paragraph 3 | 1. All provisions of paragraphs 1 to 8 included. 2. Strength tests on mechanicals couplings of simple design may be replaced by virtual tests. 3. Paragraphs 3.6.1 (Strength test), 3.6.2 (Resistance to buckling) and 3.6.3 (Resistance to bending moment) only.
52 | Directive 2001/85/EC | 1. Annex I 2. Annex IV Strength of superstructure | 1. Point 7.4.5 Stability test under the conditions specified in the Appendix to Annex I. 2. Appendix 4 — Verification of strength of the superstructure by calculation.
52A | Regulation (EC) No 661/2009 UNECE Regulation No 107 | Annex 3 | Paragraph 7.4.5 (calculation method)
52B | Regulation (EC) No 661/2009 UNECE Regulation No 66 | Annex 9 | Computer simulation of rollover test on complete vehicle as an equivalent approval method
57 | Directive 2000/40/EC | Paragraph 3 of Annex 5 to UNECE Regulation 93. | Resistance under a horizontal force and deflection measurement.
57A | Regulation (EC) No 661/2009 UNECE Regulation No 93 | Annex 5, Paragraph 3. | Resistance under a horizontal force and deflection measurement.
ANNEX V

Amendments to Regulation (EU) No 1003/2010
Annex II to Regulation (EU) No 1003/2010 is amended as follows:
1. point 1.2.1.2.1 is replaced by the following:
1.2.1.2.1.
The plate shall be perpendicular (± 5°) to the longitudinal plane of the vehicle.
2. points 1.2.1.5.1 and 1.2.1.5.2 are replaced by the following:
1.2.1.5.1.

If the height of the upper edge of the plate from the ground surface does not exceed 1,20 m, the plate shall be visible in the whole space included within the following four planes:
  - the two vertical planes touching the two lateral edges of the plate and forming an angle measured outwards to the left and to the right of the plate of 30° in relation to the longitudinal plane, parallel to the longitudinal median plane of the vehicle, passing through the centre of the plate,
  - the plane touching the upper edge of the plate and forming an angle measured upwards of 15° with the horizontal,
  - the horizontal plane through the lower edge of the plate.
1.2.1.5.2.

If the height of the upper edge of the plate from the ground surface exceeds 1,20 m, the plate shall be visible in the whole space included within the following four planes:
  - the two vertical planes touching the two lateral edges of the plate and forming an angle measured outwards to the left and to the right of the plate of 30° in relation to the longitudinal plane, parallel to the longitudinal median plane of the vehicle, passing through the centre of the plate,
  - the plane touching the upper edge of the plate and forming an angle measured upwards of 15° with the horizontal,
  - the plane touching the lower edge of the plate and forming an angle measured downwards of 15° with the horizontal.
3. point 1.2.3 is replaced by the following:
1.2.3.
Whenever it is declared by the vehicle manufacturer that a vehicle is suitable for towing loads (point 2.11.5 of Annex I to Directive 2007/46/EC) and if the space for mounting the rear registration plate may as a result be (partly) obscured within the planes of geometrical visibility due to the permitted and/or recommended installation of any mechanical coupling device, this shall be noted in the test report and stated on the EC type-approval certificate. Furthermore, vehicle type-approval shall not be granted unless measures are taken to ensure that such mechanical coupling device, if installed and not in use, can be removed or repositioned only without the use of any tools, including release keys.
ANNEX VI

Amendments to Regulation (EU) No 109/2011
Regulation (EU) No 109/2011 is amended as follows:
1. in Annex I, Part I, footnote (*) is deleted;
2. in Annex IV, point 0.1 is replaced by the following:
0.1.

Category N and O vehicles, with the exception of off-road vehicles as defined in Annex II to Directive 2007/46/EC, shall be constructed and/or fitted with spray suppression systems in such a way as to meet the requirements laid down in this Annex. In the case of chassis/cab vehicles, these requirements may only be applied to the wheels covered by the cab.
At the manufacturer's discretion, for vehicles of category N1, N2 with a permissible maximum laden mass not exceeding 7,5 tonnes, O1 and O 2, the requirements of Commission Regulation (EU) No 1009/2010 as set out for vehicle category M1 may be applied instead of the requirements of this Annex. In such a case, the information document shall include all the particulars relevant to wheel guards as laid down in Article 3(2) of that Regulation.
ANNEX VII

Amendments to Regulation (EU) No 458/2011
Annex I to Regulation (EU) No 458/2011 is amended as follows:
in Part 2, Addendum, point 3.2 is replaced by the following:
3.2.
Vehicle category N1: yes/no (1), type 1/2/3/4/5 (1)
.
OJ L 263, 9.10.2007, p. 1.
OJ L 200, 31.7.2009, p. 1.
Council Directive 71/320/EEC of 26 July 1971 on the approximation of the laws of the Member States relating to the braking devices of certain categories of motor vehicles and of their trailers (OJ L 202, 6.9.1971, p. 37).
OJ L 185, 13.7.2012, p. 24.
OJ L 304, 20.11.2010, p. 21.
Commission Directive 2010/19/EU of 9 March 2010 amending, for the purposes of adaptation to technical progress in the field of spray-suppression systems of certain categories of motor vehicles and their trailers, Council Directive 91/226/EEC, and Directive 2007/46/EC of the European Parliament and of the Council (OJ L 72, 20.3.2010, p. 17).
Commission Regulation (EU) No 1003/2010 of 8 November 2010 concerning type-approval requirements for the space for mounting and the fixing of rear registration plates on motor vehicles and their trailers and implementing Regulation (EC) No 661/2009 of the European Parliament and of the Council concerning type-approval requirements for the general safety of motor vehicles, their trailers and systems, components and separate technical units intended therefor (OJ L 291, 9.11.2010, p. 22).
Commission Regulation (EU) No 109/2011 of 27 January 2011 implementing Regulation (EC) No 661/2009 of the European Parliament and of the Council as regards type-approval requirements for certain categories of motor vehicles and their trailers as regards spray suppression systems (OJ L 34, 9.2.2011, p. 2).
Commission Regulation (EU) No 458/2011 of 12 May 2011 concerning type-approval requirements for motor vehicles and their trailers with regard to the installation of their tyres and implementing Regulation (EC) No 661/2009 of the European Parliament and of the Council concerning type-approval requirements for the general safety of motor vehicles, their trailers and systems, components and separate technical units intended therefor (OJ L 124, 13.5.2011, p. 11).
OJ L 310, 26.11.2010, p. 18.
Delete where not applicable.
If a part (e.g. component or separate technical unit) has been type-approved, that part need not be described if reference is made to such approval. Similarly, a part need not be described if its construction is clearly apparent from the attached diagrams or drawings. For each item for which drawings or photographs shall be attached, give numbers of the corresponding attached documents.
If the means of identification of type contains characters not relevant to describe the vehicle, component or separate technical unit types covered by this information document, such characters shall be represented in the documentation by the symbol ‘?’ (e.g. ABC??123??).
Classified according to the definitions set out in Directive 2007/46/EC Part A of Annex II.
If the means of identification of type contains characters not relevant to describe the vehicle, component or separate technical unit types covered by this information document, such characters shall be represented in the documentation by the symbol ‘?’ (e.g. ABC??123??).
As defined in Directive 2007/46/EC, Annex II, Section A.
If the means of identification of type contains characters not relevant to describe the vehicle, component or separate technical unit types covered by this information document, such characters shall be represented in the documentation by the symbol ‘?’ (e.g. ABC??123??).
As defined in Directive 2007/46/EC, Annex II, Section A.
Delete where not applicable.
Delete where not applicable.
Commission Regulation (EU) No 1008/2010 of 9 November 2010 concerning type-approval requirements for windscreen wiper and washer systems of certain motor vehicles and implementing Regulation (EC) No 661/2009 of the European Parliament and of the Council concerning type-approval requirements for the general safety of motor vehicles, their trailers and systems, components and separate technical units intended therefor (OJ L 292, 10.11.2010, p. 2).
Commission Regulation (EU) No 19/2011 of 11 January 2011 concerning type-approval requirements for the manufacturer's statutory plate and for the vehicle identification number of motor vehicles and their trailers and implementing Regulation (EC) No 661/2009 of the European Parliament and of the Council concerning type-approval requirements for the general safety of motor vehicles, their trailers and systems, components and separate technical units intended therefor (OJ L 8, 12.1.2011, p. 1).
Commission Regulation (EU) No 249/2012 of 21 March 2012 amending Regulation (EU) No 19/2011 as regards type-approval requirements for the manufacturer's statutory plate of motor vehicles and their trailers (OJ L 82, 22.3.2012, p. 1).’
Commission Regulation (EU) No 1009/2010 of 9 November 2010 concerning type-approval requirements for wheel guards of certain motor vehicles and implementing Regulation (EC) No 661/2009 of the European Parliament and of the Council concerning type-approval requirements for the general safety of motor vehicles, their trailers and systems, components and separate technical units intended therefor (OJ L 292, 10.11.2010, p. 21).’