CHAPTER III

CONFORMITY OF SUBSYSTEMS AND SAFETY COMPONENTS

Rules and conditions for affixing the CE marking
Article 21
1
The CE marking shall be affixed visibly, legibly and indelibly to the subsystem or the safety component or to its data plate. Where that is not possible or not warranted on account of the nature of the subsystem or the safety component, it shall be affixed to the packaging and to the accompanying documents.
2
The CE marking shall be affixed before the subsystem or the safety component is placed on the market.
3
The CE marking shall be followed by the identification number of the notified body involved in the production control phase. The identification number of the notified body shall be affixed by the body itself or, under its instructions, by the manufacturer or his authorised representative.
4
The CE marking and the identification number referred to in paragraph 3 may be followed by any other mark indicating a special risk or use.
5
Member States shall build upon existing mechanisms to ensure correct application of the regime governing the CE marking and shall take appropriate action in the event of improper use of that marking.