CHAPTER III

CONFORMITY OF SUBSYSTEMS AND SAFETY COMPONENTS

Rules and conditions for affixing the UK marking
Article 21
1
The UK marking shall be affixed visibly, legibly and indelibly to the subsystem or the safety component or to its data plate. Where that is not possible or not warranted on account of the nature of the subsystem or the safety component, it shall be affixed to the packaging and to the accompanying documents.
2
The UK marking shall be affixed before the subsystem or the safety component is placed on the market.
3
The UK marking shall be followed by the identification number of the notified body involved in the production control phase. The identification number of the notified body shall be affixed by the body itself or, under its instructions, by the manufacturer or his authorised representative.
4
The UK marking and the identification number referred to in paragraph 3 may be followed by any other mark indicating a special risk or use.
5. . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . .
Words in Art. 21 heading substituted (31.12.2020) by The Cableway Installations (Amendment) (EU Exit) Regulations 2019 (S.I. 2019/1347), regs. 1, 30(a); 2020 c. 1, Sch. 5 para. 1(1)
Art. 21(5) omitted (31.12.2020) by virtue of The Cableway Installations (Amendment) (EU Exit) Regulations 2019 (S.I. 2019/1347), regs. 1, 30(b); 2020 c. 1, Sch. 5 para. 1(1)
Words in Art. 21 substituted (31.12.2020) by The Cableway Installations (Amendment) (EU Exit) Regulations 2019 (S.I. 2019/1347), regs. 1, 30(a); 2020 c. 1, Sch. 5 para. 1(1)