PART II

OPERATIONAL SECURITY
TITLE 2

DATA EXCHANGE
CHAPTER 4

Data exchange between TSOs, owners of interconnectors or other lines and power generating modules connected to the transmission system

Scheduled data exchange
Article 46
1
Each SGU which is a power generating facility owner of a type B, C or D power generating module connected to the transmission system shall provide the TSO with at least the following data:
a
active power output and active power reserves amount and availability, on a day-ahead and intra-day basis;
b
without any delay, any scheduled unavailability or active power restriction;
c
any forecasted restriction in the reactive power control capability ...
d. . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . .
2
Each HVDC system operator shall provide the TSOs with at least the following data:
a
active power schedule and availability on a day-ahead and intra-day basis;
b
without delay its scheduled unavailability or active power restriction; and
c
any forecast restriction in the reactive power or voltage control capability.
3
Each AC interconnector or line operator shall provide its scheduled unavailability or active power restriction data to the TSOs.
Art. 46(1)(d) and word omitted (E.W.S.) (31.12.2020) by virtue of The Electricity Network Codes and Guidelines (System Operation and Connection) (Amendment etc.) (EU Exit) Regulations 2019 (S.I. 2019/533), reg. 1(2), Sch. 1 para. 40 (as amended by S.I. 2020/1016, regs. 1(2), 6(2)); 2020 c. 1, Sch. 5 para. 1(1)