PART II

OPERATIONAL SECURITY
TITLE 2

DATA EXCHANGE
CHAPTER 6

Data exchange between TSOs and demand facilities

Data exchange between TSOs and transmission-connected demand facilities
Article 52
1
Unless otherwise provided by the TSO, each transmission-connected demand facility owner shall provide the following structural data to the TSO:
a
electrical data of the transformers connected to the transmission system;
b
characteristics of the load of the demand facility; and
c
characteristics of the reactive power control.
2
Unless otherwise provided by the TSO, each transmission-connected demand facility owner shall provide the following data to the TSO:
a
scheduled active and forecasted reactive power consumption on a day-ahead and intraday basis, including any changes of those schedules or forecast;
b
any forecasted restriction in the reactive power control capability;
c
in case of participation in demand response, a schedule of its structural minimum and maximum power range to be curtailed ...
d. . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . .
3
Unless otherwise provided by the TSO, each transmission-connected demand facility owner shall provide the following data to the TSO in real-time:
a
active and reactive power at the connection point; and
b
the minimum and maximum power range to be curtailed.
4
Each transmission-connected demand facility owner shall describe to its TSO its behaviour at the voltage ranges referred to in Article 27.
Art. 52(2)(d) and word omitted (E.W.S.) (31.12.2020) by virtue of The Electricity Network Codes and Guidelines (System Operation and Connection) (Amendment etc.) (EU Exit) Regulations 2019 (S.I. 2019/533), reg. 1(2), Sch. 1 para. 43 (as amended by S.I. 2020/1016, regs. 1(2), 6(2)); 2020 c. 1, Sch. 5 para. 1(1)