PART III

OPERATIONAL PLANNING
TITLE 1

DATA FOR OPERATIONAL SECURITY ANALYSIS IN OPERATIONAL PLANNING

Updates of year-ahead individual ... grid models
Article 68
1
When a TSO modifies or notices a modification of its best estimates for the variables used for determining its year-ahead individual grid model established in accordance with Article 66(1), which is significant for operational security, it shall update its year-ahead individual grid model ....
2. . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . .
Words in Art. 68 heading omitted (E.W.S.) (31.12.2020) by virtue of The Electricity Network Codes and Guidelines (System Operation and Connection) (Amendment etc.) (EU Exit) Regulations 2019 (S.I. 2019/533), reg. 1(2), Sch. 1 para. 52(2) (as amended by S.I. 2020/1016, regs. 1(2), 6(2)); 2020 c. 1, Sch. 5 para. 1(1)
Words in Art. 68(1) omitted (E.W.S.) (31.12.2020) by virtue of The Electricity Network Codes and Guidelines (System Operation and Connection) (Amendment etc.) (EU Exit) Regulations 2019 (S.I. 2019/533), reg. 1(2), Sch. 1 para. 52(3) (as amended by S.I. 2020/1016, regs. 1(2), 6(2)); 2020 c. 1, Sch. 5 para. 1(1)
Art. 68(2) omitted (E.W.S.) (31.12.2020) by virtue of The Electricity Network Codes and Guidelines (System Operation and Connection) (Amendment etc.) (EU Exit) Regulations 2019 (S.I. 2019/533), reg. 1(2), Sch. 1 para. 52(4) (as amended by S.I. 2020/1016, regs. 1(2), 6(2)); 2020 c. 1, Sch. 5 para. 1(1)