CHAPTER III

ALLOCATION OF FIRM CAPACITY PRODUCTS

Applied capacity unit
Article 10
The capacity offered shall be expressed in energy units per unit of time. The following units shall be used: kWh/h or kWh/d. In case of kWh/d a flat flow rate over the gas day is assumed.