Requirements and test procedures for GB type-approval of 112-based eCall in-vehicle system components
Article 6
1
GB type-approval of a 112-based eCall in-vehicle system component shall be subject to the component passing the tests laid down in Annex I and complying with the relevant requirements in that Annex.
2
For the purposes of paragraph 1, only the verification procedure for components laid down in point 2.8 of Annex I shall apply after the individual parts are subjected to the test referred to in point 2.3 of this Annex.
3
Upon request of the manufacturer, a component may additionally be tested by the technical service for compliance with the requirements set out in Annexes IV, VI and VII that are relevant to the functionalities of the component. Compliance with those requirements shall be indicated on the type-approval certificate issued in accordance with Article 3(3) of Commission Implementing Regulation (EU) 2017/78 .
Commission Implementing Regulation (EU) 2017/78 of 15 July 2016 establishing administrative provisions for the EC type-approval of motor vehicles with respect to their 112-based eCall in-vehicle systems and uniform conditions for the implementation of Regulation (EU) 2015/758 of the European Parliament and of the Council with regard to the privacy and data protection of users of such systems (see page 26 of this Official Journal).
Words in Art. 6 heading substituted (31.12.2022 at 11.00 p.m.) by The Road Vehicles and Non-Road Mobile Machinery (Type-Approval) (Amendment and Transitional Provisions) (EU Exit) Regulations 2022 (S.I. 2022/1273), regs. 1(2), 79(2)
Words in Art. 6 substituted (31.12.2022 at 11.00 p.m.) by The Road Vehicles and Non-Road Mobile Machinery (Type-Approval) (Amendment and Transitional Provisions) (EU Exit) Regulations 2022 (S.I. 2022/1273), regs. 1(2), 79(2)