SCHEDULE 1

Euro Standards for Compression Ignition Engine Vehicles
Regulation 2(1)(a)
In this schedule vehicle categories M1 to M3 include ambulances, hearses and motor caravans.
Table 1

Euro 6 standards for compression ignition engine vehicles
Vehicle category | Reference mass of vehicle, where relevant (kg) | Limit values for CO (mg/km) | Limit values for NOx (mg/km) | Limit values for THC+NOx (mg/km) | Limit values for PM | Limit values for PN (#/km) | Appropriate Test
category M1 | not exceeding 2610 | 500 | 80 | 170 | 4.5 | 6 x 10 | Type I
category M2 | not exceeding 2610 | 500 | 80 | 170 | 4.5 | 6 x 10 | Type I
category N1 sub-class (i) | not exceeding 1305 | 500 | 80 | 170 | 4.5 | 6 x 10 | Type I
category N1 sub-class (ii) | exceeding 1305 and not exceeding 1760 | 630 | 105 | 195 | 4.5 | 6 x 10 | Type I
category N1 sub-class (iii) | exceeding 1760 | 740 | 125 | 215 | 4.5 | 6 x 10 | Type I
category N2 | not exceeding 2610 | 740 | 125 | 215 | 4.5 | 6 x 10 | Type I
Table 2

Euro VI standards for compression ignition engine vehicles
Vehicle category | Reference mass of vehicle, where relevant (kg) | Limit values for CO (mg/kWh) | Limit values for NOx (mg/kWh) | Limit values for NH3 (ppm) | Limit values for PM (mg/kWh) | ParticleMass Number(#kWh) | Appropriate Test
category M1 | exceeding 2610 | 1500 | 400 | 10 | 10 | 6 x 10 | WHSC
category M1 | exceeding 2610 | 4000 | 460 | 10 | 10 | 6 x 10 | WHTC
category M2 | exceeding 2610 | 1500 | 400 | 10 | 10 | 6 x 10 | WHSC
category M2 | exceeding 2610 | 4000 | 460 | 10 | 10 | 6 x 10 | WHTC
category M3 | exceeding 2610 | 1500 | 400 | 10 | 10 | 6 x 10 | WHSC
category M3 | exceeding 2610 | 4000 | 460 | 10 | 10 | 6 x 10 | WHTC
category N2 | exceeding 2610 | 1500 | 400 | 10 | 10 | 6 x 10 | WHSC
category N2 | exceeding 2610 | 4000 | 460 | 10 | 10 | 6 x 10 | WHTC
category N3 | exceeding 2610 | 1500 | 400 | 10 | 10 | 6 x 10 | WHSC
category N3 | exceeding 2610 | 4000 | 460 | 10 | 10 | 6 x 10 | WHTC
SCHEDULE 2

Euro Standards for Positive Ignition Engine Vehicles
Regulation 2(1)(b)
In this schedule vehicle categories M1 to M3 include ambulances, hearses and motor caravans.
Table 1

Euro 4 standards for positive ignition engine vehicles
Vehicle category | Reference mass of vehicle, where relevant (kg) | Maximum mass of vehicle, where relevant (kg) | Limit values for CO (g/km) | Limit values for NOx (g/km) | Limit values for HC (g/km) | Appropriate Test
category M1 | | not exceeding 2500 | 1 | 0.08 | 0.1 | Type I
category M1 | not exceeding 1305 | exceeding 2500 | 1 | 0.08 | 0.1 | Type I
category M1 | exceeding 1305 and not exceeding 1760 | exceeding 2500 | 1.81 | 0.1 | 0.13 | Type I
category M1 | exceeding 1760 | exceeding 2500 | 2.27 | 0.11 | 0.16 | Type I
category M2 | | not exceeding 2500 | 1 | 0.08 | 0.1 | Type I
category M2 | exceeding 1305 and not exceeding 1760 | exceeding 2500 and not exceeding 3500 | 1.81 | 0.1 | 0.13 | Type I
category M2 | exceeding 1760 | exceeding 2500 and not exceeding 3500 | 2.27 | 0.16 | 0.11 | Type I
category M2 | not exceeding 2840 | exceeding 3500 | 2.27 | 0.16 | 0.11 | Type I
category N1 sub-class (i) | not exceeding 1305 | | 1 | 0.08 | 0.1 | Type I
category N1 sub-class (ii) | exceeding 1305 and not exceeding 1760 | | 1.81 | 0.1 | 0.13 | Type I
category N1 sub-class (iii) | exceeding 1760 | | 2.27 | 0.11 | 0.16 | Type I
category N2 | not exceeding 2840 | | 2.27 | 0.11 | 0.16 | Type I
Table 2

Euro IV standards for positive ignition engine vehicles
Vehicle category | Reference mass of vehicle, where relevant (kg) | Limit values for CO (g/kWh) | Limit values for HC (g/kWh) | Limit values for NOx (g/kWh) | Limit values for PM (g/kWh) | Limit values for NMHC (g/kWh) | Limit values for CH4 (g/kWh) | Limit values for smoke(m-1) | Appropriate Test
category M3 | exceeding 2610 | 1.5 | 0.46 | 3.5 | 0.02 | | | 0.5 | ESC and ELR
category M3 | exceeding 2610 | 4.0 | | 3.5 | | 0.55 | 1.1 | | ETC
category N3 | exceeding 2610 | 1.5 | 0.46 | 3.5 | 0.02 | | | 0.5 | ESC and ELR
category N3 | exceeding 2610 | 4.0 | | 3.5 | | 0.55 | 1.1 | | ETC
SCHEDULE 3

Euro Standards for Mopeds and Motorcycles
Regulation 2(1)(c)
Table

Euro 3 standards for mopeds and motorcycles
Vehicle category | Class (engine capacity in cubic centimetres) | Limit values for CO (g/km) | Limit values for HC (g/km) | Limit values for NOx (g/km) | Limit values for THC+NOx (g/km) | Appropriate Test
moped | | 1 | | | 1.2 | Type I for mopeds and motorcycles and Type II for mopeds and motorcycles
motorcycle | not exceeding 150 | 2 | 0.8 | 0.15 | | Type I for mopeds and motorcycles and Type II for mopeds and motorcycles
motorcycle | exceeding 150 | 2 | 0.3 | 0.15 | | Type I for mopeds and motorcycles and Type II for mopeds and motorcycles
SCHEDULE 4

Penalty Charge Rates
Regulation 4

Table
Vehicle | Description | Initial penalty charge | First surcharge | Second surcharge | Third Surcharge | Fourth Surcharge
Column 1 | Column 2 | Column 3 | Column 4 | Column 5 | Column 6 | Column 7
light passenger vehicle | | £60 | £60 | £180 | £420 | £420
minibus | | £60 | £60 | £180 | £420 | £900
bus or coach | | £60 | £60 | £180 | £420 | £900
light goods vehicle | | £60 | £60 | £180 | £420 | £420
heavy goods vehicle | vehicle within category N2 | £60 | £60 | £180 | £420 | £900
heavy goods vehicle | vehicle within category N3 | £60 | £60 | £180 | £420 | £900
ambulance | | £60 | £60 | £180 | £420 | £420
hearse | | £60 | £60 | £180 | £420 | £420
motor caravan | | £60 | £60 | £180 | £420 | £420
mopeds or motorcycles | | £60 | £60 | £180 | £420 | £420