PART 2

PRINCIPAL POWERS

Limits of deviation
5
1
In carrying out the authorised development for which it is granted development consent by article 3(1) (development consent etc. granted by the Order) except as provided in paragraphs (2), (3) and (4) the undertaker may—
a
deviate laterally from the lines or situations of the authorised development shown on the Works Plans within the limits of deviation relating to a Work shown on those plans and subject to Requirement 42 carry out construction activities for the purpose of the authorised development anywhere within the Order limits; and
b
deviate vertically from the levels of the authorised development shown on the sections—
i
to any extent upwards not exceeding 4 metres in respect of the overhead lines;
ii
to any extent upwards not exceeding 10% of the maximum height shown on the relevant design drawings in respect of the substations, cable sealing end compounds and permanent bridges; and
iii
to any extent downwards as may be found to be necessary or convenient.
2
Pylon LD32 must be constructed 40 metres northwards (plus or minus 5 metres northwards or southwards to allow local ground conditions to be taken into account) from the position shown on the Works Plans within the limits of deviation relating to that Work as shown on those plans, together with a corresponding decrease or increase in height of pylon LD32 and of pylon LD31 as appropriate comprised in Work
No.
1D shown in the sections (Drawing No 13/NG/0271 – 01_13205_84 revision B, Sheet 4).
3
Pylon LD51 (and adjacent spans LD50 to LD51 to LD52) forming part of the authorised development comprised in Work No. 1E must not deviate laterally westwards from the lines or situations of the authorised development shown on the Works Plans section D, sheets 5 and 6 within the limits of deviation relating to that Work shown on those plans such that the overhead line cannot be constructed closer to Moorland Park than the centre line of Work No. 1E.
4
Pylons LD109 – LD113 must be constructed in accordance with the dimensions shown on drawing No 01_13205_84 showing increased pylon height within Bristol Port, Avonmouth, in order to provide a minimum 20.7m vertical ground clearance for the spans between pylons LD109 to LD113.
Art. 5(2) substituted (21.7.2017) by The National Grid (Hinkley Point C Connection Project) (Correction) Order 2017 (S.I. 2017/786), arts. 1, 3, Sch.