SCHEDULE 1

List of Specified Dangerous Goods
Regulation 8(1)
1
The dangerous goods referred to in regulation 8(1) are:
a
more than 10 kilograms of explosives in Division 1.1 or 250 kilograms in aggregate of explosives in Division 1.2, 1.3 and 1.5; when explosives in Division 1.1 are carried simultaneously in the vessel with explosives in Division 1.2, 1.3 or 1.5, the overall limit is 10 kilograms;
b
more than 25 tonnes of sodium chlorate or potassium chlorate, or more than 500 tonnes of ammonium nitrate of Class 5.1;
c
bulk liquefied gases of Class 2, including the remnants of such gases which remain after their discharge from a tank which has not subsequently been gas-freed or inerted;
d
bulk liquids of Class 3, including the remnants of such liquids which remain after their discharge from a tank which has not subsequently been gas-freed or inerted;
e
bulk liquids of Classes 4, 5, 6.1 and 8 of UN Packing Groups I and II in the UN list;
f
bulk liquids of Class 6.1, UN Packing Group III in the UN list, if such liquids have a harmful inhalation risk.
2
In paragraph 1—
- “UN List” means the version of the UN list referred to in Chapter 3.2 of the IMDG Code as updated from time to time.
Sch. 1 para. 1 in force at 1.10.2016, see reg. 1
Sch. 1 para. 2 in force at 1.10.2016, see reg. 1