PART 2

Works Provisions

Limits of deviation
7
1
Save in relation to the drainage works, where paragraph (2) applies, the undertaker may—
a
in respect of the location of any work comprised in the authorised development deviate laterally from the lines or situations shown on the works plans to the extent of the limits of deviation for that work shown on those plans; and
b
in respect of Work No.1 deviate vertically;
i
for each or any part of Work No. 1 referred to in column 1 of the table below, to the limit upwards specified in relation to that part of Work No.1 in column 2 of that table;
ii
to any extent downwards as may be found necessary or practical to a maximum depth of 70 metres below the surface of the ground; and
iii
except that subparagraph (i) does not apply to those parts of Work No.1 that are built within the Goxhill AGI and the Paull AGI.
Table 1
(1) Scheduled Work | (2) Upwards Vertical Deviation Limits
| Below ground level (m) | Below watercourses (m) | Below true clean bed (m) | Below highways (m)
1A | 1.2 | 1.7 | Not applicable | Not applicable
1B | 4.0 | 1.7 | 7.0 | Not applicable
1C | 1.2 | 1.7 | Not applicable | 2.0
c
deviate or place Work Nos. 2, 3, 4, 7 and 8 laterally and vertically to the limits set for these works in paragraph 1 of Schedule 1.
d
carry out construction activities for the purposes of the authorised project anywhere within the Order limits.
2
The undertaker may construct the drainage works anywhere within the Order limits.
Art. 7 in force at 15.9.2016, see art. 1