Penalties
52
In Schedule 13, Part 2, Chapter 1—
a
in the entry for article 42(1), after “42(1)” insert “(other than sub-paragraph (b)(ii))”;
b
after the entry for article 44(2) insert—
44(5) | Requirement for certificate of release to service for equipment installed on or in a non-EASA aircraft after its overhaul, repair, modification or inspection
;
c
after the entry for article 51 insert—
54(1) | Aircraft maintenance programme
55 | Aircraft to be managed by approved continuing airworthiness management organisation and maintained by approved maintenance organisation
;
d
for the entry for article 77(1) and (3) to (6) substitute—
77(1) and (3) to (7) | Requirements for aircraft to carry equipment
;
e
for the entry for article 78(4) substitute—
78A(3) | Carriage of equipment
;
f
for the two entries relating to article 80 substitute—
80 | Requirement for— 1. operation of airborne collision avoidance system 2. training in operation of airborne collision avoidance system
; and
g
for the two entries relating to article 119 substitute—
119 | Carriage and use of equipment Vibration health monitoring system to be operated in accordance with approved procedures
.
Art. 52 in force at 14.12.2017, see art. 1