ANNEX

DISCRETE PROCESSES AND OPERATIONAL PARAMETERS ASSOCIATED WITH START-UP AND SHUT-DOWN PERIODS
2.

Operational parameters
2.1.
Oxygen content of the flue gases.
2.2.
Flue gas temperature.
2.3.
Steam pressure.
2.4.
For heat producing plants: enthalpy and heat transfer fluid rate.
2.5.
For liquid and gas fired plants: fuel flow rate, specified as a percentage of the rated fuel flow capacity.
2.6.
For steam boiler plants: temperature of steam at the exit of the boiler.