Definitions and interpretation
Article 2
For the purposes of this Decision the following definitions apply:
1. ‘minimum start-up load for stable generation’ means the minimum load compatible with the steady operation of the generating combustion plant following start-up initiation after which the plant is able to safely and reliably deliver its output to a network, grid, heat accumulator or industrial site;
2. ‘minimum shut-down load for stable generation’ means the minimum load at which point the plant can no longer safely and reliably deliver its output to a network, grid, heat accumulator or industrial site and is considered to be shutting down.
3. For the purpose of this Decision a reference to a provision of a Directive is to be read as a reference to that provision in so far as it has been transposed into the law of any part of the United Kingdom.
Words in Art. 2 heading inserted (31.12.2020) by The Air Quality (Miscellaneous Amendment and Revocation of Retained Direct EU Legislation) (EU Exit) Regulations 2018 (S.I. 2018/1407), regs. 1, 8(2)(a); 2020 c. 1, Sch. 5 para. 1(1)
Art. 2(3) inserted (31.12.2020) by The Air Quality (Miscellaneous Amendment and Revocation of Retained Direct EU Legislation) (EU Exit) Regulations 2018 (S.I. 2018/1407), regs. 1, 8(2)(b); 2020 c. 1, Sch. 5 para. 1(1)