Article 1
The values relating to the performance of manufacturers, as confirmed...
Article 2
This Decision is addressed to the following individual manufacturers: AUDI...
ANNEX
Explanatory notes to Tables 1 and 2
Column A:
Column B:
Column C:
Column D:
Column E:
Column F:
Column G:
Column I:
Commission Implementing Decision
of 17 December 2013
confirming or amending the average specific emissions of CO2 and specific emissions targets for manufacturers of new light commercial vehicles for the calendar year 2012 pursuant to Regulation (EU) No 510/2011 of the European Parliament and of the Council
(notified under document C(2013) 9184)
(Only the Dutch, English, French, German, Italian, Polish, Portuguese, Romanian, Spanish, and Swedish texts are authentic)
(2013/807/EU)
THE EUROPEAN COMMISSION,
Having regard to the Treaty on the Functioning of the European Union,
Having regard to Regulation (EU) No 510/2011 of the European Parliament and of the Council of 11 May 2011 setting emission performance standards for new light commercial vehicles as part of the Union’s integrated approach to reduce CO2 emissions from light-duty vehicles , and in particular Article 8(6) and Article 10(1) thereof,
Whereas:
(1)
The Commission is required, pursuant to Article 8(6) of Regulation (EU) No 510/2011, to confirm or amend each year the average specific emissions of CO2 and the specific emissions target for each manufacturer of light commercial vehicles in the Union. On that basis, the Commission is to determine whether manufacturers and pools of manufacturers formed in accordance with Article 7(1) of that Regulation have complied with their specific emissions targets in accordance with Article 4 of that Regulation.
(2)
For the calendar years 2012 and 2013, the specific emissions targets are not binding and the Commission should therefore calculate indicative targets. As those indicative targets will serve as indicators to manufacturers of the effort required to reach the mandatory target in 2014, it is appropriate to determine the average specific emissions of CO2 of manufacturers for 2012 and 2013 in accordance with the requirements set out in the third paragraph of Article 4 of Regulation (EU) No 510/2011 and take into account 70 % of the manufacturer’s new light commercial vehicles registered in that year.
(3)
The detailed data to be used for the calculation of the average specific emissions of CO2 and the specific emissions targets are set out in point 1 of Part A of Annex II to Regulation (EU) No 510/2011 and are based on Member States’ registrations of new light commercial vehicles.
(4)
Where light commercial vehicles are type-approved in a multi-stage process, point 7 of Part B of Annex II to Regulation (EU) No 510/2011 requires that the manufacturer of the base vehicle take responsibility for the CO2 emissions of the completed vehicle. Pending the applicability of the procedure for determining CO2 emissions from this category of vehicles as provided for in Section 5 of Annex XII to Commission Regulation (EC) No 692/2008 , the Commission should calculate the specific emissions target for manufacturers of base vehicles using the mass in running order of the completed vehicle as defined in Article 3(1)(g) of Regulation (EU) No 510/2011 and should use the specific emissions of CO2 of the base vehicle in accordance with the second paragraph of Article 4 of that Regulation.
(5)
The complete datasets for all Member States were made available to the Commission by the end of March 2013. Where, as a result of the verification of the data by the Commission, it was evident that certain data were missing or manifestly incorrect, the Commission contacted the Member States concerned and, subject to the agreement of those Member States, adjusted or completed the data accordingly. Where no agreement could be reached with a Member State, the provisional data of that Member State were not adjusted.
(6)
It should be noted that several Member States have not been able to distinguish between complete and completed light commercial vehicles in their current monitoring systems. As a consequence, the 2012 data for light commercial vehicles should be considered incomplete with regard to the monitoring of vehicles type-approved in a multi-stage process. In order to ensure a full and accurate monitoring of the CO2 emissions and the technical data relating in particular to multi-stage vehicles, it is necessary to adjust the monitoring systems both at Union and Member State level. Therefore, the final values as confirmed in this Decision should not be considered fully representative of the CO2 emissions performance of the new vehicle fleet in 2012.
(7)
On 18 June 2013, the Commission published the provisional data on light commercial vehicles and notified 60 manufacturers of the provisional calculations of their average specific emissions of CO2 in 2012 and their specific emissions targets in accordance with Article 8(4) of Regulation (EU) No 510/2011. Manufacturers were asked to verify the data and to notify the Commission of any errors within three months of receipt of the notification in accordance with the Article 8(5) of that Regulation. Four manufacturers notified the Commission that they accepted the preliminary data without corrections whilst 24 manufacturers submitted notifications of errors.
(8)
For the 36 manufacturers that did not notify any errors in the datasets, the provisional data and provisional calculations of the average specific emissions of CO2 and the specific emissions targets should be confirmed without adjustments.
(9)
The Commission has verified the corrections notified by the manufacturers and the respective justifications and the datasets have been adjusted as appropriate.
(10)
In the case of records with missing or incorrect identification parameters, such as type, variant, version code or type-approval number, the fact that manufacturers cannot verify or correct those records should be taken into account. As a consequence, it is appropriate to apply an error margin to the CO2 emissions and mass values in those records.
(11)
The error margin should be calculated as the difference between the distances to the specific emissions target expressed as the specific emissions targets subtracted from the average emissions calculated including and excluding those registrations that cannot be verified by the manufacturers. Regardless of whether that difference is positive or negative, the error margin should always improve the distance to the target of the manufacturer.
(12)
The average specific emissions of CO2 from new light commercial vehicles registered in 2012, the specific emissions targets and the difference between those two values should be confirmed or amended accordingly,
HAS ADOPTED THIS DECISION:
OJ L 145, 31.5.2011, p. 1.
Commission Regulation (EC) No 692/2008 of 18 July 2008 implementing and amending Regulation (EC) No 715/2007 of the European Parliament and of the Council on type-approval of motor vehicles with respect to emissions from light passenger and commercial vehicles (Euro 5 and Euro 6) and on access to vehicle repair and maintenance information (OJ L 199, 28.7.2008, p. 1).